<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="16.51" x2="72.695" y2="16.51" width="0" layer="20"/>
<wire x1="72.695" y1="16.51" x2="72.695" y2="74.92" width="0" layer="20"/>
<wire x1="72.695" y1="74.92" x2="-1.27" y2="74.92" width="0" layer="20"/>
<wire x1="-1.27" y1="74.92" x2="-1.27" y2="16.51" width="0" layer="20"/>
<text>A0</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>modular-muse.com</text>
<text>5V</text>
<text>GND</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>GND</text>
<text>GND</text>
<text>D2</text>
<text>D3~</text>
<text>D4</text>
<text>D5~</text>
<text>D7</text>
<text>D6~</text>
<text>D8</text>
<text>D9~</text>
<text>D10~</text>
<text>D11~</text>
<text>D12</text>
<text>D13</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
</plain>
<libraries>
<library name="jif">
<packages>
<package name="MYCON2_HEAD15-NOSS">
</package>
<package name="CLIPPY">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="jif" package="MYCON2_HEAD15-NOSS" value="NANO"/>
<element name="U$8" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$9" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$2" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$3" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$4" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$5" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$6" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$10" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$11" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$12" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$13" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$14" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$15" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$16" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="2.2K" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="U$7" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$17" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$18" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$19" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$20" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="U$21" library="jif" package="CLIPPY" value="CLIPPY"/>
<element name="JP5" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="JP6" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="R5" library="SparkFun-Passives" package="1/6W-RES" value="10k"/>
<element name="R6" library="SparkFun-Passives" package="1/6W-RES" value="10k"/>
<element name="R7" library="SparkFun-Passives" package="1/6W-RES" value="10k"/>
<element name="R8" library="SparkFun-Passives" package="1/6W-RES" value="10k"/>
</elements>
<signals>
<signal name="D13">
<contactref element="U$1" pad="D13"/>
<contactref element="U$16" pad="1"/>
<contactref element="U$16" pad="2"/>
<contactref element="2.2K" pad="P$1"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="A0"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="A1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="A2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="A3"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="A4">
<contactref element="U$1" pad="A4"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$7" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="A5">
<contactref element="U$1" pad="A5"/>
<contactref element="U$17" pad="1"/>
<contactref element="U$17" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="A6">
<contactref element="U$1" pad="A6"/>
<contactref element="U$18" pad="1"/>
<contactref element="U$18" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="A7">
<contactref element="U$1" pad="A7"/>
<contactref element="U$19" pad="1"/>
<contactref element="U$19" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V"/>
<contactref element="2.2K" pad="P$2"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$8" pad="1"/>
<contactref element="U$8" pad="2"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$9" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$20" pad="1"/>
<contactref element="U$20" pad="2"/>
<contactref element="U$21" pad="1"/>
<contactref element="U$21" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="D2"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="D3"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="D4"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="D5"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="D6"/>
<contactref element="U$6" pad="1"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="D7"/>
<contactref element="U$10" pad="1"/>
<contactref element="U$10" pad="2"/>
</signal>
<signal name="D8">
<contactref element="U$1" pad="D8"/>
<contactref element="U$11" pad="1"/>
<contactref element="U$11" pad="2"/>
</signal>
<signal name="D9">
<contactref element="U$1" pad="D9"/>
<contactref element="U$12" pad="1"/>
<contactref element="U$12" pad="2"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="D10"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$13" pad="2"/>
</signal>
<signal name="D11">
<contactref element="U$1" pad="D11"/>
<contactref element="U$14" pad="1"/>
<contactref element="U$14" pad="2"/>
</signal>
<signal name="D12">
<contactref element="U$1" pad="D12"/>
<contactref element="U$15" pad="1"/>
<contactref element="U$15" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
