<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.37" y2="0" width="0" layer="20"/>
<wire x1="12.37" y1="0" x2="12.37" y2="15.23" width="0" layer="20"/>
<wire x1="12.37" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-5050-IC">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH">
</package>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-LED" package="LED-TRICOLOR-5050-IC" value="WS2811">
<attribute name="PROD_ID" value="DIO-11598"/>
</element>
<element name="U2" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2"/>
<element name="-" library="SparkFun-Connectors" package="1X03" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="-" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="-" pad="2"/>
</signal>
<signal name="DI">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="2" route="any" routetag="DI"/>
</signal>
<signal name="DO">
<contactref element="-" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
