<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<circle x="20.32" y="20.32" radius="20.32" width="0.0254" layer="20"/>
<text>SENSOR</text>
<text>BTN</text>
<text>PWR</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>H</text>
<text>D</text>
<text>PZO</text>
<text>Rev C</text>
<text>GND</text>
</plain>
<libraries>
<library name="00-SGAMF">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="0204/8">
<description>RESISTOR</description>
</package>
<package name="JR-DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="JR-KK-04">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
<package name="JR-KK-02">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
<package name="0805">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOIC-14">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IR" library="00-SGAMF" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="00-SGAMF" package="JR-DIL04" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="00-SGAMF" package="JR-DIL04" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="00-SGAMF" package="0204/8" value="IR">
<attribute name="VALUE"/>
</element>
<element name="E$1" library="00-SGAMF" package="JR-KK-04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="00-SGAMF" package="JR-KK-02" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="00-SGAMF" package="JR-KK-02" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="00-SGAMF" package="0204/8" value="51">
<attribute name="VALUE"/>
</element>
<element name="PIC16F684" library="SparkFun-DigitalIC" package="SOIC-14" value="">
<attribute name="NAME"/>
</element>
<element name="C2" library="00-SGAMF" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PZO" library="00-SGAMF" package="JR-KK-02" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="00-SGAMF" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="00-SGAMF" package="0204/8" value="5K">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$7">
<contactref element="Q2" pad="P$1"/>
<contactref element="Q2" pad="P$2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="S$1">
<contactref element="Q1" pad="P$1"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="E$3" pad="P$2"/>
<contactref element="Q2" pad="P$3"/>
<contactref element="PIC16F684" pad="14"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="P$3"/>
<contactref element="E$1" pad="P$2"/>
<contactref element="E$2" pad="P$2"/>
<contactref element="PZO" pad="P$2"/>
<contactref element="ICSP" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="S$2">
<contactref element="IR" pad="K"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="5VDC">
<contactref element="E$3" pad="P$1"/>
<contactref element="IR" pad="A"/>
<contactref element="E$1" pad="P$3"/>
<contactref element="C2" pad="2"/>
<contactref element="PIC16F684" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="S$4">
<contactref element="E$1" pad="P$1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="S$5">
<contactref element="Q1" pad="P$4"/>
<contactref element="PIC16F684" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="ICSPDAT">
<contactref element="E$2" pad="P$1"/>
<contactref element="PIC16F684" pad="13"/>
<contactref element="ICSP" pad="3"/>
</signal>
<signal name="S$3">
<contactref element="E$1" pad="P$4"/>
<contactref element="PIC16F684" pad="11"/>
</signal>
<signal name="S$8">
<contactref element="PIC16F684" pad="7"/>
<contactref element="PZO" pad="P$1"/>
</signal>
<signal name="S$9">
<contactref element="Q2" pad="P$4"/>
<contactref element="PIC16F684" pad="8"/>
</signal>
<signal name="ICSPCLK">
<contactref element="ICSP" pad="4"/>
<contactref element="PIC16F684" pad="12"/>
</signal>
<signal name="S$23">
</signal>
<signal name="S$22">
</signal>
<signal name="S$17">
</signal>
<signal name="S$92">
</signal>
<signal name="S$95">
</signal>
<signal name="ICSPVPP">
<contactref element="ICSP" pad="1"/>
<contactref element="PIC16F684" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
