<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>silpstream.com</text>
<wire x1="1.905" y1="15.875" x2="28.575" y2="15.875" width="0.254" layer="20"/>
<wire x1="28.575" y1="15.875" x2="28.575" y2="1.905" width="0.254" layer="20"/>
<wire x1="28.575" y1="1.905" x2="1.905" y2="1.905" width="0.254" layer="20"/>
<wire x1="1.905" y1="1.905" x2="1.905" y2="15.875" width="0.254" layer="20"/>
<text>Melzi2MiniPanel v1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X10_NOSILK">
</package>
<package name="2X3-NS">
</package>
<package name="2X5_NOSILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MINIPANEL" library="SparkFun-Connectors" package="2X10_NOSILK" value="M10X2NOSILK"/>
<element name="JP1" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="2X5_NOSILK" value="M05X2NO_SILK"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="MINIPANEL" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="MINIPANEL" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="MINIPANEL" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="MINIPANEL" pad="7"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="3V3">
<contactref element="MINIPANEL" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="MINIPANEL" pad="11"/>
</signal>
<signal name="LCD_BL">
<contactref element="MINIPANEL" pad="13"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="BEEP">
<contactref element="MINIPANEL" pad="15"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="ENC_B">
<contactref element="MINIPANEL" pad="17"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="ENC_A">
<contactref element="MINIPANEL" pad="19"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="SD_DETECT">
<contactref element="MINIPANEL" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="MINIPANEL" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SD_SS">
<contactref element="MINIPANEL" pad="6"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="MINIPANEL" pad="8"/>
</signal>
<signal name="RESET">
<contactref element="MINIPANEL" pad="10"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="MINIPANEL" pad="12"/>
</signal>
<signal name="LCD_CS">
<contactref element="MINIPANEL" pad="14"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="LCD_A0">
<contactref element="MINIPANEL" pad="16"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="STOP">
<contactref element="MINIPANEL" pad="18"/>
</signal>
<signal name="ENC_SW">
<contactref element="MINIPANEL" pad="20"/>
<contactref element="JP2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
