<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<polygon width="0.4064" layer="46">
<vertex x="58.42" y="17.78"/>
<vertex x="66.04" y="17.78" curve="90"/>
<vertex x="68.58" y="20.32" curve="90"/>
<vertex x="66.04" y="22.86"/>
<vertex x="58.42" y="22.86"/>
<vertex x="58.42" y="30.48"/>
<vertex x="66.04" y="30.48" curve="90"/>
<vertex x="68.58" y="33.02" curve="90"/>
<vertex x="66.04" y="35.56"/>
<vertex x="58.42" y="35.56"/>
<vertex x="58.42" y="43.18"/>
<vertex x="66.04" y="43.18" curve="90"/>
<vertex x="68.58" y="45.72" curve="90"/>
<vertex x="66.04" y="48.26"/>
<vertex x="58.42" y="48.26"/>
<vertex x="58.42" y="63.5"/>
<vertex x="50.8" y="63.5"/>
<vertex x="50.8" y="69.85" curve="90"/>
<vertex x="48.26" y="72.39" curve="90"/>
<vertex x="45.72" y="69.85"/>
<vertex x="45.72" y="63.5"/>
<vertex x="38.1" y="63.5"/>
<vertex x="38.1" y="69.85" curve="90"/>
<vertex x="35.56" y="72.39" curve="90"/>
<vertex x="33.02" y="69.85"/>
<vertex x="33.02" y="63.5"/>
<vertex x="25.4" y="63.5"/>
<vertex x="25.4" y="48.26"/>
<vertex x="17.78" y="48.26" curve="90"/>
<vertex x="15.24" y="45.72" curve="90"/>
<vertex x="17.78" y="43.18"/>
<vertex x="25.4" y="43.18"/>
<vertex x="25.4" y="35.56"/>
<vertex x="17.78" y="35.56" curve="90"/>
<vertex x="15.24" y="33.02" curve="90"/>
<vertex x="17.78" y="30.48"/>
<vertex x="25.4" y="30.48"/>
<vertex x="25.4" y="22.86"/>
<vertex x="17.78" y="22.86" curve="90"/>
<vertex x="15.24" y="20.32" curve="90"/>
<vertex x="17.78" y="17.78"/>
<vertex x="25.4" y="17.78"/>
<vertex x="25.4" y="12.7"/>
<vertex x="33.02" y="12.7"/>
<vertex x="33.02" y="6.35" curve="90"/>
<vertex x="35.56" y="3.81" curve="90"/>
<vertex x="38.1" y="6.35"/>
<vertex x="38.1" y="12.7"/>
<vertex x="45.72" y="12.7"/>
<vertex x="45.72" y="6.35" curve="90"/>
<vertex x="48.26" y="3.81" curve="90"/>
<vertex x="50.8" y="6.35"/>
<vertex x="50.8" y="12.7"/>
<vertex x="58.42" y="12.7"/>
</polygon>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BEL/P">
<description>&lt;b&gt;LI BATTERY&lt;/b&gt; Sonnenschein&lt;p&gt;
SL-340 P</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="D2" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value="RES-10698"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value="RES-10698"/>
</element>
<element name="G1" library="battery" package="BEL/P" value="SL-340/P"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="K"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="K"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="V+">
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="G1" pad="+"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="G1" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
