<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="61.595" y2="0" width="0" layer="20"/>
<wire x1="61.595" y1="0" x2="61.595" y2="44.45" width="0" layer="20"/>
<wire x1="61.595" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<hole x="1.905" y="5.3975" drill="2.3876"/>
<hole x="13.97" y="33.655" drill="2.3876"/>
<hole x="48.895" y="37.7825" drill="2.3876"/>
<hole x="55.88" y="12.065" drill="2.3876"/>
<text>GND</text>
<text>BATT</text>
<text>TX</text>
<text>RX</text>
<text>GPS</text>
<text>CAN</text>
<text>RX</text>
<text>TX</text>
<text>VSS</text>
<text>VDD</text>
<text>V0</text>
<text>RS</text>
<text>RW</text>
<text>E</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>A</text>
<text>R</text>
<text>G</text>
<text>B</text>
<text>LCD</text>
<text>SCK</text>
<text>SO</text>
<text>MI</text>
<text>MO</text>
<text>SI</text>
<text>SS</text>
<text>TACH</text>
<text>SPI</text>
<text>RESET</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>12V</text>
<text>5V</text>
<text>3V3</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>A</text>
<text>B</text>
<text>SW</text>
<text>C</text>
<text>5V</text>
<text>S</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>AUX I/O</text>
<text>ENC</text>
<text>Sensor
Interface
Teensy 3.1
Rev. 1.0</text>
<text>I2C</text>
<text>ONE-WIRE</text>
<text>C3</text>
<text>C4</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>ANALOG</text>
<text>Sensor
Interface
Teensy 3.1
Rev. 1.0</text>
</plain>
<libraries>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_ALLPINS">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SMA-DIODE_ALT">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="EIA6032">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
<package name="1X05">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL6-SMD">
<description>&lt;b&gt;DIL 6 SMD&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/pf/4N/4N35-M.html</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_ALLPINS" value="TEENSY_3.1_ALL_PINS_AND_PADS"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="100">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1206" value="100">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1206" value="10K">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1206" value="10K">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1206" value="10K">
<attribute name="NAME"/>
</element>
<element name="VREG" library="SparkFun-PowerIC" package="SOT223" value="AP1117">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="EIA6032" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="EIA6032" value=""/>
<element name="LCD" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="FACTORY_RESET" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="ONE_WIRE" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="1206" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="I2C" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="POWER" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="GPS" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE_ALT" value="1N4007">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE_ALT" value="1N4007">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="1206" value="1k">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="1206" value="330">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SMA-DIODE_ALT" value="5.1V">
<attribute name="NAME"/>
</element>
<element name="OK1" library="optocoupler" package="DIL6-SMD" value="H11L1MS">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="CAN" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="R10" library="SparkFun-Resistors" package="1206" value="91k">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="TACH" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="AUX_IO" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="1206" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="1206" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="1206" value="91k">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="1206" value="18k">
<attribute name="NAME"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A_IN1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="A_IN2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="TEST1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="TEST2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="SPI1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="SPI2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="ENC1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="ENC2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="AGND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="VREG" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="C3" pad="P$2"/>
<contactref element="LCD" pad="1"/>
<contactref element="FACTORY_RESET" pad="1"/>
<contactref element="FACTORY_RESET" pad="2"/>
<contactref element="ONE_WIRE" pad="3"/>
<contactref element="POWER" pad="2"/>
<contactref element="GPS" pad="4"/>
<contactref element="OK1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="OK1" pad="5"/>
<contactref element="R11" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="TEST1" pad="1"/>
<contactref element="ENC1" pad="1"/>
</signal>
<signal name="LCD_V0">
<contactref element="U$1" pad="A14"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="VBAT">
<contactref element="U$1" pad="VBAT"/>
<contactref element="GPS" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="3.3V1"/>
<contactref element="U$1" pad="3.3V2"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="R7" pad="1"/>
<contactref element="OK1" pad="6"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="TEST2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="VIN"/>
<contactref element="C2" pad="1"/>
<contactref element="VREG" pad="2"/>
<contactref element="C4" pad="P$1"/>
<contactref element="LCD" pad="2"/>
<contactref element="LCD" pad="11"/>
<contactref element="ONE_WIRE" pad="1"/>
<contactref element="GPS" pad="5"/>
<contactref element="TEST2" pad="1"/>
</signal>
<signal name="VUSB">
<contactref element="U$1" pad="VUSB"/>
</signal>
<signal name="PROGRAM">
<contactref element="U$1" pad="PGM"/>
</signal>
<signal name="AREF">
<contactref element="U$1" pad="AREF"/>
</signal>
<signal name="ONE_WIRE">
<contactref element="U$1" pad="33"/>
<contactref element="ONE_WIRE" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="FACTORY_RESET">
<contactref element="U$1" pad="32"/>
<contactref element="FACTORY_RESET" pad="3"/>
</signal>
<signal name="SDA1">
<contactref element="U$1" pad="30"/>
<contactref element="I2C" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="SCL1">
<contactref element="U$1" pad="29"/>
<contactref element="I2C" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="CAN_TX">
<contactref element="U$1" pad="3"/>
<contactref element="CAN" pad="1"/>
</signal>
<signal name="CAN_RX">
<contactref element="U$1" pad="4"/>
<contactref element="CAN" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="11"/>
<contactref element="SPI1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="12"/>
<contactref element="SPI2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="13"/>
<contactref element="SPI2" pad="2"/>
</signal>
<signal name="ENC_SW">
<contactref element="U$1" pad="14/A0"/>
<contactref element="ENC2" pad="2"/>
</signal>
<signal name="ENC_A">
<contactref element="U$1" pad="16/A2"/>
<contactref element="ENC1" pad="2"/>
</signal>
<signal name="ENC_B">
<contactref element="U$1" pad="15/A1"/>
<contactref element="ENC2" pad="1"/>
</signal>
<signal name="TACH">
<contactref element="U$1" pad="17/A3"/>
<contactref element="OK1" pad="4"/>
</signal>
<signal name="AF_RATIO">
<contactref element="U$1" pad="18/A4"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="MAP">
<contactref element="U$1" pad="19/A5"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="AUX1">
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="AUX2">
<contactref element="R28" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="U$1" pad="20/A6"/>
</signal>
<signal name="AUX3">
<contactref element="R29" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="U$1" pad="21/A7"/>
</signal>
<signal name="AUX4">
<contactref element="R30" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="U$1" pad="22/A8"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="3"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="N$46">
<contactref element="Q2" pad="3"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="N$47">
<contactref element="Q3" pad="3"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="N$48">
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="R1" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="R3" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="RED">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="GREEN">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="BLUE">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="LCD_RS">
<contactref element="U$1" pad="2"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="LCD_RW">
<contactref element="LCD" pad="5"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="LCD_E">
<contactref element="LCD" pad="6"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="LCD_D4">
<contactref element="U$1" pad="24"/>
<contactref element="LCD" pad="7"/>
</signal>
<signal name="LCD_D5">
<contactref element="LCD" pad="8"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="LCD_D6">
<contactref element="LCD" pad="9"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="LCD_D7">
<contactref element="LCD" pad="10"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="GPS_RX">
<contactref element="GPS" pad="3"/>
<contactref element="U$1" pad="0"/>
</signal>
<signal name="GPS_TX">
<contactref element="GPS" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="POWER" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R10" pad="2"/>
<contactref element="TEST1" pad="2"/>
</signal>
<signal name="SS">
<contactref element="U$1" pad="10"/>
<contactref element="SPI1" pad="1"/>
</signal>
<signal name="AUX5">
<contactref element="R31" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="U$1" pad="23/A9"/>
</signal>
<signal name="N$1">
<contactref element="VREG" pad="3"/>
<contactref element="C3" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="C"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="R9" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="TACH_SIGNAL">
<contactref element="D2" pad="A"/>
<contactref element="TACH" pad="1"/>
</signal>
<signal name="BATT_VOLTS">
<contactref element="U$1" pad="A13"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="AUTO_DIM">
<contactref element="U$1" pad="A12"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="COOLANT_TEMP">
<contactref element="U$1" pad="A11"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="OIL_PRESS">
<contactref element="U$1" pad="31"/>
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="FUEL_LEVEL">
<contactref element="U$1" pad="A10"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="AUX1_SIGNAL">
<contactref element="AUX_IO" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="AUX2_SIGNAL">
<contactref element="AUX_IO" pad="2"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="AUX3_SIGNAL">
<contactref element="AUX_IO" pad="3"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="AUX4_SIGNAL">
<contactref element="AUX_IO" pad="4"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="AUX5_SIGNAL">
<contactref element="AUX_IO" pad="5"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="AUTO_DIM_SIGNAL">
<contactref element="R14" pad="2"/>
<contactref element="A_IN1" pad="1"/>
</signal>
<signal name="MAP_SIGNAL">
<contactref element="R24" pad="2"/>
<contactref element="A_IN2" pad="3"/>
</signal>
<signal name="COOLANT_TEMP_SIGNAL">
<contactref element="R16" pad="2"/>
<contactref element="A_IN1" pad="2"/>
</signal>
<signal name="FUEL_LEVEL_SIGNAL">
<contactref element="R18" pad="2"/>
<contactref element="A_IN1" pad="3"/>
</signal>
<signal name="OIL_PRESS_SIGNAL">
<contactref element="R20" pad="2"/>
<contactref element="A_IN2" pad="1"/>
</signal>
<signal name="AF_RATIO_SIGNAL">
<contactref element="R22" pad="2"/>
<contactref element="A_IN2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
