<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>CPPM</text>
<text>GND</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>RST</text>
<wire x1="0" y1="22.225" x2="0" y2="1.27" width="0" layer="20"/>
<text>XL7105-CL</text>
<text>XL7105-CL RC RX</text>
<text>20150206</text>
<wire x1="0" y1="22.225" x2="1.27" y2="23.495" width="0" layer="20" curve="-90"/>
<wire x1="17.78" y1="23.495" x2="19.05" y2="22.225" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="0" x2="19.05" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="23.495" x2="17.78" y2="23.495" width="0" layer="20"/>
<wire x1="19.05" y1="22.225" x2="19.05" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="brandon">
<packages>
<package name="XL7105-CL">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="1X07_LONGPADS">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="rcl" package="R0805" value="330">
<attribute name="NAME"/>
</element>
<element name="LED" library="adafruit" package="CHIP-LED0805" value="blue 3.3v">
<attribute name="NAME"/>
</element>
<element name="IC3" library="v-reg" package="SOT223" value="LD1117AS33"/>
<element name="C1" library="rcl" package="C0805K" value="100nf">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0805K" value="4.7uf">
<attribute name="NAME"/>
</element>
<element name="U$2" library="brandon" package="XL7105-CL" value="XL7105CL"/>
<element name="U$1" library="SparkFun" package="SO08-EIAJ" value="ATTINY45/85">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X07_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="BIND" library="SparkFun" package="SJ_2S-NO" value="BIND JUMPER">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="IC3" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="C1" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$2" pad="16"/>
<contactref element="U$2" pad="17"/>
<contactref element="U$2" pad="18"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP2" pad="5"/>
<contactref element="BIND" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="13"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="12"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="CPPM">
<contactref element="U$1" pad="2"/>
<contactref element="JP2" pad="7"/>
<contactref element="BIND" pad="1"/>
</signal>
<signal name="GIO1">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="LED" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="7"/>
<contactref element="LED" pad="C"/>
<contactref element="U$2" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
