<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="-1.999653125" y1="3.6061375" x2="6.04243125" y2="3.6061375" width="0" layer="20"/>
<wire x1="6.04243125" y1="3.6061375" x2="6.043365625" y2="21.001078125" width="0" layer="20"/>
<wire x1="6.043365625" y1="21.001078125" x2="-2.031359375" y2="21.001075" width="0" layer="20"/>
<wire x1="-2.031359375" y1="21.001075" x2="-1.999653125" y2="3.6061375" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="IPOD_MALE_CONNECTOR">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="IPOD_MALE_CONNECTOR" value="IPOD_CONNECTOR_MALE"/>
<element name="GND" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D-" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D+" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ACC" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="U$1" pad="25"/>
<contactref element="D-" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="27"/>
<contactref element="D+" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="13"/>
<contactref element="RX" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="12"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="23"/>
<contactref element="5V" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="21"/>
<contactref element="ACC" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="GND1" pad="1"/>
<contactref element="GND" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
