<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.64" y2="0" width="0" layer="20"/>
<wire x1="40.64" y1="0" x2="40.64" y2="11.43" width="0" layer="20"/>
<wire x1="40.64" y1="11.43" x2="0" y2="11.43" width="0" layer="20"/>
<wire x1="0" y1="11.43" x2="0" y2="0" width="0" layer="20"/>
<text>SCL</text>
<text>SDA</text>
<text>PACK</text>
<text>BATT</text>
<text>Li-Po BQ27200</text>
<text>(C)Lt_Flash, 2015</text>
<text>Fuel Gauge</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X03">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DRK_S-PDSO-N10">
<description>&lt;b&gt;DRK (S-PDSO-N10)&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. bq27010.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Passives" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="texas" package="DRK_S-PDSO-N10" value="BQ27210">
<attribute name="OC_NEWARK" value="30M3431"/>
<attribute name="MPN" value="BQ27210DRKR"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1534540"/>
</element>
<element name="RS" library="SparkFun-Passives" package="1206" value="0.02">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP3" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="PACK+">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="PACK-">
<contactref element="R2" pad="2"/>
<contactref element="RS" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="RBI">
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="4"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="5"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="SRP">
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SRN">
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="PP"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="PP@1"/>
<contactref element="IC1" pad="PP@2"/>
<contactref element="IC1" pad="PP@3"/>
<contactref element="IC1" pad="PP@4"/>
<contactref element="IC1" pad="PP@5"/>
<contactref element="IC1" pad="PP@6"/>
<contactref element="IC1" pad="PP@7"/>
<contactref element="IC1" pad="PP@8"/>
<contactref element="IC1" pad="PP@9"/>
<contactref element="IC1" pad="PP@10"/>
<contactref element="RS" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="BAT">
<contactref element="C3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
