<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="3.1242" x2="49.12" y2="1.397" width="0.0254" layer="20"/>
<wire x1="55.44" y1="1.397" x2="70.358" y2="1.397" width="0.0254" layer="20"/>
<wire x1="70.358" y1="1.397" x2="70.358" y2="65.5828" width="0.0254" layer="20"/>
<wire x1="70.358" y1="65.5828" x2="55.44" y2="65.5828" width="0.0254" layer="20"/>
<wire x1="49.12" y1="65.5828" x2="7.112" y2="64.3382" width="0.0254" layer="20"/>
<hole x="27.2796" y="5.0292" drill="3.2"/>
<hole x="27.2796" y="61.97" drill="3.2"/>
<hole x="67.28" y="62.56" drill="3.2"/>
<hole x="67.28" y="4.447" drill="3.2"/>
<wire x1="0" y1="40.132" x2="0" y2="3.1242" width="0.0254" layer="20"/>
<wire x1="49.12" y1="1.397" x2="49.12" y2="5.13" width="0.0254" layer="20"/>
<wire x1="55.44" y1="1.397" x2="55.44" y2="5.13" width="0.0254" layer="20"/>
<wire x1="49.12" y1="5.13" x2="55.44" y2="5.13" width="0.0254" layer="20" curve="-180"/>
<wire x1="49.12" y1="61.87" x2="49.12" y2="65.5828" width="0.0254" layer="20"/>
<wire x1="55.44" y1="61.87" x2="55.44" y2="65.5828" width="0.0254" layer="20"/>
<wire x1="55.44" y1="61.87" x2="49.12" y2="61.87" width="0.0254" layer="20" curve="-180"/>
<wire x1="7.112" y1="40.132" x2="7.112" y2="64.3382" width="0.0254" layer="20"/>
<wire x1="7.112" y1="40.132" x2="0" y2="40.132" width="0.0254" layer="20"/>
<text>Receiver</text>
<text>Version 1.1</text>
<text>By: D. Keefe</text>
<text>Charge Rate Jumper</text>
<text>Open: 100 mA</text>
<text>Closed: 280 mA</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>Rocket Track</text>
<text>BLK</text>
<text>BLK</text>
</plain>
<libraries>
<library name="My_Parts">
<packages>
<package name="LED-0603">
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="SOT23-3">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="CON-BATT">
</package>
<package name="SW-A11AH">
</package>
<package name="USB-WURTH-629105136821">
<description>Micro USB Package</description>
</package>
<package name="CON-0.1-6PIN">
</package>
<package name="BUZZER-12MM">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-1">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D3" library="My_Parts" package="LED-0603" value="GREEN">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="TLMG1100-GS08"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="My_Parts" package="LED-0603" value="RED">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="TLMS1100-GS08"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="My_Parts" package="0603-RES" value="301">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="CRCW0603301RFKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="301"/>
</element>
<element name="R1" library="My_Parts" package="0603-RES" value="301">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="CRCW0603301RFKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="301"/>
</element>
<element name="C5" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="My_Parts" package="0603-CAP" value="1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C105K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="My_Parts" package="SOT23-3" value="TPS3839">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="TPS3839G33DBZR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="My_Parts" package="SOT23-5" value="TPS73632">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="TPS73632DBVT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-RF" package="XBEE-1" value="XBEE-1B1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="My_Parts" package="CON-BATT" value="CONN-BATT">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="D2" library="My_Parts" package="LED-0603" value="RED">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="TLMS1100-GS08"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="My_Parts" package="0603-RES" value="301">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="CRCW0603301RFKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="301"/>
</element>
<element name="C2" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="My_Parts" package="0603-CAP" value="1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C105K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-RF" package="XBEE-1" value="XBEE-1B1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="C6" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="My_Parts" package="0603-CAP" value="0.1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="My_Parts" package="SOT23-5" value="MAX1555">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="MAX1555EZK+T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="My_Parts" package="SW-A11AH" value="SWITCH-A11AH">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="A11AH"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="My_Parts" package="USB-WURTH-629105136821" value="USB-MICROB">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="629105136821"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="J2" library="My_Parts" package="CON-0.1-6PIN" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIST" value="Mouser"/>
<attribute name="PN" value="22-28-4065"/>
</element>
<element name="J1" library="My_Parts" package="CON-0.1-6PIN" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIST" value="Mouser"/>
<attribute name="PN" value="22-28-4065"/>
</element>
<element name="LS1" library="My_Parts" package="BUZZER-12MM" value="BUZZER-12MM">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="PB-12N23P-03Q"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="My_Parts" package="SOT23-3" value="FDV301N">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="FDV301N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="My_Parts" package="0603-CAP" value="1uF">
<attribute name="DIST" value="Digikey"/>
<attribute name="PN" value="C0603C105K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U4" pad="2"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U4" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="D1" pad="C"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="5"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="J4" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="XBEE_RX">
<contactref element="SJ2" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="ASSOC">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="D3" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C8" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="D3" pad="A"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="LS1" pad="+"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="SJ3" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="VBUS">
<contactref element="U3" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBATT_SW">
<contactref element="C9" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="XBEE_TX">
<contactref element="SJ1" pad="1"/>
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="BT_TX">
<contactref element="SJ2" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="BT_RX">
<contactref element="U2" pad="3"/>
<contactref element="SJ1" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="3"/>
<contactref element="LS1" pad="-"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="15"/>
<contactref element="Q1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
