<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="29.19" y2="0" width="0" layer="20"/>
<wire x1="29.19" y1="0" x2="29.19" y2="25.07" width="0" layer="20"/>
<wire x1="29.19" y1="25.07" x2="0" y2="25.07" width="0" layer="20"/>
<wire x1="0" y1="25.07" x2="0" y2="0" width="0" layer="20"/>
<hole x="13.335" y="13.97" drill="2.8"/>
<hole x="13.335" y="3.81" drill="2.8"/>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>5x20mm</text>
<text>Stir Bus</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_SMD">
</package>
<package name="1X02">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FUSE_HOLDER_5X20MM">
<description>&lt;b&gt;Fuse Holder&lt;/b&gt; 5x20 mm&lt;p&gt;
Source: User LBR Version 2.05</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="PROD_ID" value="CONN-08106"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="F1" library="fuse" package="FUSE_HOLDER_5X20MM" value="FUSEBLANK_5X20MM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="JP5" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="JP6" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="VIN0"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="F1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="GND"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP4" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="JP3" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
