<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.585" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="24.38" y2="0" width="0" layer="20"/>
<wire x1="24.38" y1="0" x2="25.38" y2="1" width="0" layer="20" curve="90"/>
<wire x1="25.38" y1="1" x2="25.38" y2="16.585" width="0" layer="20"/>
<wire x1="25.38" y1="16.585" x2="24.38" y2="17.585" width="0" layer="20" curve="90"/>
<wire x1="24.38" y1="17.585" x2="1" y2="17.585" width="0" layer="20"/>
<wire x1="1" y1="17.585" x2="0" y2="16.585" width="0" layer="20" curve="90"/>
<text>OFF/ON</text>
<text>DataGate v1.0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIPSWITCH-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H"/>
<element name="JP2" library="SparkFun-Connectors" package="USB-A-S" value="USB-A-S"/>
<element name="SW1" library="SparkFun-Electromechanical" package="DIPSWITCH-02" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="POWER">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="D-"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="3"/>
<contactref element="JP2" pad="D-"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="D+"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SW1" pad="4"/>
<contactref element="JP2" pad="D+"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="VBUS"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="VBUS"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="JP1" pad="GND"/>
<contactref element="JP2" pad="GND"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
