<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>VCC</text>
<text>GND</text>
<text>D7</text>
<text>D8</text>
<text>D9</text>
<text>Relay Board v0.1b</text>
<text>Georgian Borca
2015</text>
<text>+</text>
<text>-</text>
<text>5V</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="transistor-pnp">
<description>&lt;b&gt;PNP Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="Itead_BP_110825.lbr">
<packages>
<package name="RELAY">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="DP8049_V1">
</package>
<package name="LOGO_FLAME">
<description>12x16 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="adafruit" package="SMADIODE" value=""/>
<element name="D2" library="adafruit" package="SMADIODE" value=""/>
<element name="D3" library="adafruit" package="SMADIODE" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-pnp" package="TO92" value="BC557">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-pnp" package="TO92" value="BC557">
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-pnp" package="TO92" value="BC557">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Itead_BP_110825.lbr" package="RELAY" value="RELAY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Itead_BP_110825.lbr" package="RELAY" value="RELAY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="Itead_BP_110825.lbr" package="RELAY" value="RELAY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="dp_devices" package="DP8049_V1" value=""/>
<element name="PAD1" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD2" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD3" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD4" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD5" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD6" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD7" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD8" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD9" library="wirepad" package="3,81/1,4" value=""/>
<element name="U$6" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="U$3" library="dp_devices" package="LOGO_FLAME" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="R6" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="2"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="Q1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="Q2" pad="3"/>
<contactref element="U2" pad="2"/>
<contactref element="LED2" pad="A"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="Q3" pad="3"/>
<contactref element="LED3" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="K"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LED2" pad="K"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LED3" pad="K"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="4"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="5"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="1"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="4"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="5"/>
<contactref element="PAD6" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="PAD9" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="PAD7" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="U3" pad="1"/>
<contactref element="PAD8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
