<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<hole x="3.175" y="38.1" drill="2.9464"/>
<hole x="22.225" y="38.1" drill="2.9464"/>
<wire x1="0.635" y1="41.275" x2="0.635" y2="34.925" width="0" layer="20"/>
<wire x1="0.635" y1="34.925" x2="5.08" y2="34.925" width="0" layer="20"/>
<wire x1="5.08" y1="3.81" x2="20.32" y2="3.81" width="0" layer="20"/>
<wire x1="20.32" y1="34.925" x2="24.765" y2="34.925" width="0" layer="20"/>
<wire x1="24.765" y1="34.925" x2="24.765" y2="41.275" width="0" layer="20"/>
<wire x1="0.635" y1="41.275" x2="24.765" y2="41.275" width="0" layer="20"/>
<text>5V</text>
<text>3V3</text>
<text>ANALOG IN</text>
<text>REV LIMIT</text>
<text>FOR LIMIT</text>
<text>CAN</text>
<text>CAN</text>
<text>QUAD ENCODER</text>
<text>L(G)</text>
<text>H(Y)</text>
<text>Developed by</text>
<text>TechHOUNDS 868</text>
<text>H(Y)</text>
<text>H(Y)</text>
<text>L(G)</text>
<text>L(G)</text>
<text>S</text>
<text>S</text>
<text>S</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>X</text>
<text>A</text>
<text>+</text>
<text>B</text>
<wire x1="5.08" y1="3.81" x2="5.08" y2="34.925" width="0" layer="20"/>
<wire x1="20.32" y1="3.81" x2="20.32" y2="34.925" width="0" layer="20"/>
</plain>
<libraries>
<library name="custom">
<packages>
<package name="5X2-0.05&quot;">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X05">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_3">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="custom" package="5X2-0.05&quot;" value="5X2-0.05&quot;"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="120"/>
<element name="JP4" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="LED1" library="led" package="CHIP-LED0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="120"/>
</elements>
<signals>
<signal name="ANALOG_IN">
<contactref element="U$1" pad="3"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="QUAD_B">
<contactref element="U$1" pad="5"/>
<contactref element="JP4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="QUAD_A">
<contactref element="U$1" pad="7"/>
<contactref element="JP4" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="QUAD_INDEX">
<contactref element="U$1" pad="9"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="LIMIT_REV">
<contactref element="U$1" pad="8"/>
<contactref element="JP7" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="LIMIT_FOR">
<contactref element="U$1" pad="4"/>
<contactref element="JP6" pad="1"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="1"/>
<contactref element="SJ1" pad="3"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="10"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="CAN_L">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CAN_H">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R4" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
