<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="18.645996875" y1="33.772" x2="7.324103125" y2="33.772" width="0" layer="20"/>
<wire x1="7.324103125" y1="33.772" x2="4.318" y2="30.765896875" width="0" layer="20" curve="90"/>
<wire x1="4.318" y1="30.765896875" x2="4.318" y2="7.3419" width="0" layer="20"/>
<wire x1="4.318" y1="7.3419" x2="5.3099" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="5.3099" y1="6.35" x2="20.101403125" y2="6.35" width="0" layer="20"/>
<wire x1="20.101403125" y1="6.35" x2="21.133" y2="7.381596875" width="0" layer="20" curve="90"/>
<wire x1="21.133" y1="7.381596875" x2="21.133" y2="31.284996875" width="0" layer="20"/>
<wire x1="21.133" y1="31.284996875" x2="18.645996875" y2="33.772" width="0" layer="20" curve="90"/>
<text>1</text>
<text>1</text>
<text>D-PAK CHOPRA</text>
<text>PAD</text>
<text>PAD</text>
</plain>
<libraries>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="TO254P1490X508-4N">
</package>
<package name="TO170P1490X508-6N">
</package>
</packages>
</library>
<library name="-LarsFaves">
<description>I2C header</description>
<packages>
<package name="1X06_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Microchip_By_element14_Batch_1" package="TO254P1490X508-4N" value="MCP1827S-3302E/EB">
<attribute name="PACKAGE" value="DDPAK-3"/>
<attribute name="OC_NEWARK" value="88K5609"/>
<attribute name="MPN" value="MCP1827S-3302E/EB"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1840844"/>
</element>
<element name="U2" library="Microchip_By_element14_Batch_1" package="TO170P1490X508-6N" value="MCP1827-5002E/ET">
<attribute name="PACKAGE" value="DDPAK-5"/>
<attribute name="OC_NEWARK" value="88K5599"/>
<attribute name="MPN" value="MCP1827-5002E/ET"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1840846"/>
</element>
<element name="JP1" library="-LarsFaves" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
