<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="78.74" y1="0" x2="78.74" y2="25.4" width="0.2032" layer="20"/>
<wire x1="78.74" y1="25.4" x2="0" y2="25.4" width="0.2032" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="78.74" y2="0" width="0.2032" layer="20"/>
<text>D0</text>
<text>D1</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>CONTRAST</text>
<text>SWITCH</text>
<text>+</text>
<text>5V</text>
<text>P_EOC</text>
<text>GND</text>
<text>P_XCLR</text>
<text>T_INT1</text>
<text>3.3V</text>
<text>SDA</text>
<text>M_DRDY</text>
<text>A_INT1</text>
<text>SCL</text>
<text>ATMEGA328P-PU</text>
<text>C</text>
<text>2</text>
<text>T</text>
<text>1</text>
<text>Offroad
CPU</text>
<text>http://camte.ch/offroad-cpu</text>
<text>-</text>
<text>A5</text>
<text>A4</text>
<text>D2</text>
<text>D3</text>
<text>D9</text>
<text>D13</text>
<text>D12</text>
<text>D11</text>
<text>v1.1.0</text>
<text>10uF</text>
<text>10uF</text>
<text>0.1uF</text>
<text>CAMERON</text>
<text>TECH</text>
<text>+</text>
<text>-</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>REGULATOR</text>
<text>POWER</text>
<text>DISPLAY</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="DIL28-3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-4-PTH">
</package>
<package name="1X04">
</package>
<package name="1X10">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TRIM_POT_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-16X2_NOHOLES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun" package="DIL28-3" value="ATmega328-DIP-Prgrammed">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Displays" package="LCD-16X2_NOHOLES" value="LCD-16X2NOHOLES"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Electromechanical" package="TRIM_POT_PTH" value="10k">
<attribute name="VALUE"/>
</element>
<element name="SWITCH-JST" library="SparkFun-Connectors" package="JST-4-PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="SWITCH" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL2" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="">
<attribute name="VALUE"/>
</element>
<element name="5VREG" library="v-reg" package="78XXS" value="">
<attribute name="VALUE"/>
</element>
<element name="SENSOR" library="SparkFun-Connectors" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="U1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="R2" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="5VREG" pad="OUT"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="SENSOR" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="8"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="SWITCH" pad="1"/>
<contactref element="5VREG" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="SENSOR" pad="3"/>
<contactref element="SWITCH-JST" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="19"/>
<contactref element="SWITCH-JST" pad="3"/>
<contactref element="SWITCH" pad="2"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="18"/>
<contactref element="SWITCH" pad="3"/>
<contactref element="SWITCH-JST" pad="2"/>
</signal>
<signal name="DB7">
<contactref element="U1" pad="14"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="DB6">
<contactref element="U1" pad="13"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="DB5">
<contactref element="U1" pad="12"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="DB4">
<contactref element="U1" pad="11"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="E">
<contactref element="U1" pad="6"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="RS">
<contactref element="U1" pad="4"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="BL-EN">
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="R/W">
<contactref element="U1" pad="5"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="BL-A">
<contactref element="U1" pad="15"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="17"/>
<contactref element="SWITCH-JST" pad="1"/>
<contactref element="SWITCH" pad="4"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="SENSOR" pad="10"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="25"/>
<contactref element="SENSOR" pad="9"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="26"/>
<contactref element="SENSOR" pad="6"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="27"/>
<contactref element="SENSOR" pad="5"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="28"/>
<contactref element="SENSOR" pad="4"/>
</signal>
<signal name="V0">
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="16"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="21"/>
<contactref element="SENSOR" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C4" pad="1"/>
<contactref element="5VREG" pad="IN"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="INT0">
<contactref element="IC1" pad="4"/>
<contactref element="SENSOR" pad="7"/>
</signal>
<signal name="INT1">
<contactref element="IC1" pad="5"/>
<contactref element="SENSOR" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
