<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.63" y2="0" width="0" layer="20"/>
<wire x1="60.63" y1="0" x2="60.63" y2="30.47" width="0" layer="20"/>
<wire x1="60.63" y1="30.47" x2="0" y2="30.47" width="0" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="21.59" x2="55.88" y2="21.59" width="0.4064" layer="20"/>
<wire x1="55.88" y1="21.59" x2="55.88" y2="8.89" width="0.4064" layer="20"/>
<wire x1="55.88" y1="8.89" x2="17.78" y2="8.89" width="0.4064" layer="20"/>
<wire x1="17.78" y1="8.89" x2="17.78" y2="21.59" width="0.4064" layer="20"/>
<text>cutout</text>
<text>sck</text>
<text>miso</text>
<text>reset</text>
<text>vcc</text>
<text>mosi</text>
<text>gnd</text>
<text>1</text>
<text>7</text>
<text>8</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>22</text>
<text>Davewerld 2014</text>
<text>AVR programmer</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_POGO">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="2X3_POGO" value="">
<attribute name="PROD_ID" value="HW-11044"/>
</element>
<element name="1-14" library="pinhead" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="15-28" library="pinhead" package="1X14" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="P$2"/>
<contactref element="1-14" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="P$1"/>
<contactref element="15-28" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="P$3"/>
<contactref element="15-28" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="JP1" pad="P$5"/>
<contactref element="1-14" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="P$4"/>
<contactref element="15-28" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="P$6"/>
<contactref element="15-28" pad="8"/>
<contactref element="1-14" pad="8"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
