<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0.3175" y1="4.445" x2="57.1375" y2="4.445" width="0" layer="20"/>
<wire x1="57.1375" y1="4.445" x2="57.1375" y2="36.82" width="0" layer="20"/>
<wire x1="57.1375" y1="36.82" x2="0.3175" y2="36.82" width="0" layer="20"/>
<wire x1="0.3175" y1="36.82" x2="0.3175" y2="4.445" width="0" layer="20"/>
<text>ENC28J60</text>
<text>404</text>
<text>toasterpid controller
v0.9
2015</text>
<text>CONTRAST</text>
<text>LCD</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SOIC-28W">
</package>
<package name="FB603">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="1X09_LOCK">
</package>
<package name="MAGJACK">
</package>
</packages>
</library>
<library name="custom-LCD">
<packages>
<package name=".1&quot;16PIN">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="MICROSD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="dp_devices" package="SOIC-28W" value="ENC28J60">
<attribute name="NAME"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P900X900X120-32N" value="ATMEGA168P">
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="OC_NEWARK" value="03P2020"/>
<attribute name="MPN" value="ATMEGA168P-20AU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1636932"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK">
<attribute name="NAME"/>
</element>
<element name="LCD1" library="custom-LCD" package=".1&quot;16PIN" value="HD44780"/>
<element name="DAUGHTER" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="500?">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value="500?">
<attribute name="NAME"/>
</element>
<element name="L1" library="dp_devices" package="FB603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0603-RES" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="pot" package="B64Y" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0603-RES" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Passives" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="C7" library="SparkFun-Passives" package="0402-CAP" value="18pF">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0402-CAP" value="18pF">
<attribute name="NAME"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value="CRYSTAL-GROUNDED">
<attribute name="NAME"/>
</element>
<element name="SD" library="adafruit" package="MICROSD" value="MICROSD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LCD1" pad="1"/>
<contactref element="LCD1" pad="16"/>
<contactref element="DAUGHTER" pad="8"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="22"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="21"/>
<contactref element="ISP" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="10"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="M1"/>
<contactref element="J2" pad="M2"/>
<contactref element="R9" pad="A"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="RST" pad="3"/>
<contactref element="RST" pad="4"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="LCD1" pad="7"/>
<contactref element="LCD1" pad="8"/>
<contactref element="LCD1" pad="9"/>
<contactref element="LCD1" pad="10"/>
<contactref element="SD" pad="MT1"/>
<contactref element="SD" pad="MT2"/>
<contactref element="SD" pad="6"/>
</signal>
<signal name="+5V">
<contactref element="LCD1" pad="2"/>
<contactref element="DAUGHTER" pad="7"/>
<contactref element="R9" pad="E"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="LCD_CONTRAST">
<contactref element="LCD1" pad="3"/>
<contactref element="R9" pad="S"/>
</signal>
<signal name="LCD_RS">
<contactref element="LCD1" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="LCD_R/W">
<contactref element="LCD1" pad="5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="LCD_EN">
<contactref element="LCD1" pad="6"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="LCD_ANODE">
<contactref element="LCD1" pad="15"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="AVR_CLK">
<contactref element="DAUGHTER" pad="6"/>
<contactref element="ISP" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="U2" pad="8"/>
<contactref element="SD" pad="5"/>
</signal>
<signal name="D_CS">
<contactref element="DAUGHTER" pad="5"/>
<contactref element="U1" pad="9"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="D_SSR">
<contactref element="DAUGHTER" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="D_LED1">
<contactref element="DAUGHTER" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="D_LED2">
<contactref element="DAUGHTER" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="+3V3">
<contactref element="DAUGHTER" pad="9"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="28"/>
<contactref element="U2" pad="20"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="19"/>
<contactref element="ISP" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="SD" pad="4"/>
</signal>
<signal name="AVR_MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="U2" pad="7"/>
<contactref element="SD" pad="3"/>
</signal>
<signal name="PROG_RST">
<contactref element="ISP" pad="5"/>
<contactref element="U1" pad="29"/>
<contactref element="R12" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="PHY_RST">
<contactref element="U2" pad="10"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="PHY_INT">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="14"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PHY_LEDA">
<contactref element="U2" pad="27"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="PHY_LEDB">
<contactref element="U2" pad="26"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PHY_TD_N">
<contactref element="J2" pad="8"/>
<contactref element="R8" pad="1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="PHY_TD_P">
<contactref element="R7" pad="1"/>
<contactref element="J2" pad="7"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="PHY_RD_P">
<contactref element="R5" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="PHY_RD_N">
<contactref element="R6" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="RCT">
<contactref element="L1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="AVR_MISO">
<contactref element="U1" pad="16"/>
<contactref element="ISP" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="DAUGHTER" pad="4"/>
<contactref element="SD" pad="7"/>
</signal>
<signal name="AVR_CLKIN">
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="PHY_CS">
<contactref element="U2" pad="9"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R13" pad="1"/>
<contactref element="RST" pad="1"/>
<contactref element="RST" pad="2"/>
</signal>
<signal name="PHY_OSC1">
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="24"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="PHY_OSC2">
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="23"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="TDCAP">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="LCD_D4">
<contactref element="U1" pad="30"/>
<contactref element="LCD1" pad="11"/>
</signal>
<signal name="LCD_D5">
<contactref element="U1" pad="31"/>
<contactref element="LCD1" pad="12"/>
</signal>
<signal name="LCD_D6">
<contactref element="U1" pad="32"/>
<contactref element="LCD1" pad="13"/>
</signal>
<signal name="LCD_D7">
<contactref element="U1" pad="1"/>
<contactref element="LCD1" pad="14"/>
</signal>
<signal name="SD_CS">
<contactref element="SD" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="NOP">
<contactref element="U1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
