<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="46.66" y2="0" width="0" layer="20"/>
<wire x1="46.66" y1="0" x2="46.66" y2="76.19" width="0" layer="20"/>
<wire x1="46.66" y1="76.19" x2="0" y2="76.19" width="0" layer="20"/>
<wire x1="0" y1="76.19" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH-12MM">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI"/>
<element name="CC3000" library="SparkFun-Connectors" package="1X09" value="CC3000 Header"/>
<element name="RGB" library="SparkFun-Connectors" package="1X04_NO_SILK" value=""/>
<element name="IR_RECEIVE" library="SparkFun-Connectors" package="1X03" value="950nm"/>
<element name="IR_SEND" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="330"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="330"/>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM"/>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH-12MM" value="SWITCH-MOMENTARY-212MM"/>
<element name="RGB1" library="SparkFun-Connectors" package="1X04_NO_SILK" value=""/>
<element name="RGB2" library="SparkFun-Connectors" package="1X04_NO_SILK" value=""/>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="BATTERY" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="PAD1" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD2" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD3" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD4" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD5" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD6" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD7" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD8" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD9" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD10" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD11" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD12" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD13" library="wirepad" package="2,54/1,0" value=""/>
<element name="PAD14" library="wirepad" package="2,54/1,0" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="CC3000" pad="1"/>
<contactref element="ARDUINO" pad="4"/>
<contactref element="R1" pad="P$2"/>
<contactref element="RGB" pad="2"/>
<contactref element="IR_RECEIVE" pad="2"/>
<contactref element="RGB1" pad="2"/>
<contactref element="RGB2" pad="2"/>
<contactref element="S3" pad="3"/>
<contactref element="BATTERY" pad="2"/>
</signal>
<signal name="VCC3.3">
<contactref element="ARDUINO" pad="24"/>
<contactref element="CC3000" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="IR_RECEIVE" pad="3"/>
<contactref element="RGB" pad="3"/>
<contactref element="RGB1" pad="3"/>
<contactref element="RGB2" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="BATTERY" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="ARDUINO" pad="14"/>
<contactref element="CC3000" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="ARDUINO" pad="15"/>
<contactref element="CC3000" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="ARDUINO" pad="13"/>
<contactref element="CC3000" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="ARDUINO" pad="5"/>
<contactref element="CC3000" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="ARDUINO" pad="16"/>
<contactref element="CC3000" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="ARDUINO" pad="12"/>
<contactref element="CC3000" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="IR_RECEIVE" pad="1"/>
<contactref element="ARDUINO" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="ARDUINO" pad="6"/>
<contactref element="IR_SEND" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IR_SEND" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="S1" pad="1"/>
<contactref element="ARDUINO" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="P$1"/>
<contactref element="ARDUINO" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="R2" pad="P$2"/>
<contactref element="RGB" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="S2" pad="1"/>
<contactref element="ARDUINO" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="S3" pad="1"/>
<contactref element="ARDUINO" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="RGB" pad="1"/>
<contactref element="RGB2" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="RGB2" pad="1"/>
<contactref element="RGB1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="ARDUINO" pad="A4"/>
<contactref element="PAD11" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="ARDUINO" pad="A5"/>
<contactref element="PAD12" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="ARDUINO" pad="A7"/>
<contactref element="PAD13" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="ARDUINO" pad="A6"/>
<contactref element="PAD14" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="PAD9" pad="1"/>
<contactref element="ARDUINO" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="PAD1" pad="1"/>
<contactref element="ARDUINO" pad="23"/>
</signal>
<signal name="N$25">
<contactref element="ARDUINO" pad="22"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="ARDUINO" pad="20"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="ARDUINO" pad="19"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="ARDUINO" pad="18"/>
<contactref element="PAD6" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="ARDUINO" pad="17"/>
<contactref element="PAD7" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="ARDUINO" pad="21"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="PAD8" pad="1"/>
<contactref element="ARDUINO" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="PAD10" pad="1"/>
<contactref element="ARDUINO" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
