<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="32.5" x2="0" y2="27" width="0.254" layer="20"/>
<wire x1="0" y1="24" x2="0" y2="9.5" width="0.254" layer="20"/>
<wire x1="0" y1="6.5" x2="0" y2="1" width="0.254" layer="20"/>
<wire x1="1" y1="0" x2="52" y2="0" width="0.254" layer="20"/>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C6</text>
<text>C7</text>
<text>C8</text>
<text>C9</text>
<text>C10</text>
<text>C11</text>
<text>C13</text>
<text>C15</text>
<text>IC1</text>
<text>IC2</text>
<text>JP1</text>
<text>JP2</text>
<text>JP3</text>
<text>L1</text>
<text>LED1</text>
<text>LED2</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>R8</text>
<text>R9</text>
<text>R10</text>
<text>R11</text>
<text>R12</text>
<text>R13</text>
<text>R14</text>
<text>R15</text>
<text>R17</text>
<text>R19</text>
<text>R20</text>
<text>R21</text>
<text>R22</text>
<text>U$1</text>
<text>VD1</text>
<text>VD2</text>
<text>VD4</text>
<text>VD6</text>
<text>VD7</text>
<text>VD8</text>
<text>VD9</text>
<text>Y1</text>
<wire x1="53" y1="1" x2="53" y2="6.5" width="0.254" layer="20"/>
<wire x1="53" y1="9.5" x2="53" y2="24" width="0.254" layer="20"/>
<wire x1="53" y1="27" x2="53" y2="32.5" width="0.254" layer="20"/>
<wire x1="52" y1="33.5" x2="1" y2="33.5" width="0.254" layer="20"/>
<wire x1="1" y1="0" x2="0" y2="1" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="32.5" x2="1" y2="33.5" width="0.254" layer="20" curve="-90"/>
<wire x1="52" y1="33.5" x2="53" y2="32.5" width="0.254" layer="20" curve="-90"/>
<wire x1="53" y1="1" x2="52" y2="0" width="0.254" layer="20" curve="-90"/>
<wire x1="53" y1="6.5" x2="53" y2="9.5" width="0.254" layer="20" curve="-180"/>
<wire x1="53" y1="24" x2="53" y2="27" width="0.254" layer="20" curve="-180"/>
<wire x1="0" y1="27" x2="0" y2="24" width="0.254" layer="20" curve="-180"/>
<wire x1="0" y1="9.5" x2="0" y2="6.5" width="0.254" layer="20" curve="-180"/>
<text>www.coskunergan.com</text>
<text>ST-LINK V2</text>
<text>12.11.2014</text>
</plain>
<libraries>
<library name="stm32tiny">
<description>ST Cortex-M3 STM32F101/103 processor family  in LQFP100, 64, 48 and VFQPFN36 pin versions</description>
<packages>
<package name="LQFP-48">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X02">
</package>
<package name="2X5-SHROUDED">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="_MyLib">
<packages>
<package name="SOD80C">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="stm32tiny" package="LQFP-48" value=""/>
<element name="R11" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB-5PIN"/>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49U-V" value="8 MHz">
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Passives" package="0805" value="20p">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0805" value="20p">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="BLM18AG121SN1D">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1.5k">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SparkFun-PowerIC" package="SOT223" value="3V3">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="EIA3528" value="10u">
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Passives" package="EIA3528" value="10u">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="Green">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="RED">
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="510">
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="510">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="680">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="10">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="VALUE"/>
</element>
<element name="VD2" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="VD3" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="VD4" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="VD5" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="VD6" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="VD7" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="VALUE"/>
</element>
<element name="VD1" library="_MyLib" package="SOD80C" value="5V1">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="2X5-SHROUDED" value="BH-10">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="1x2">
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="36"/>
<contactref element="IC1" pad="24"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C11" pad="A"/>
<contactref element="IC2" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="VD1" pad="C"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="JP4" pad="MTN4"/>
<contactref element="JP4" pad="MTN2"/>
<contactref element="JP4" pad="GND"/>
<contactref element="JP4" pad="MTN1"/>
<contactref element="JP4" pad="MTN3"/>
<contactref element="C2" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="C"/>
<contactref element="C4" pad="C"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="20"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="VD2" pad="A"/>
<contactref element="VD3" pad="A"/>
<contactref element="VD4" pad="A"/>
<contactref element="VD5" pad="A"/>
<contactref element="VD6" pad="A"/>
<contactref element="VD7" pad="A"/>
<contactref element="VD1" pad="A"/>
<contactref element="JP3" pad="9"/>
<contactref element="R6" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="BOOT0">
<contactref element="IC1" pad="44"/>
<contactref element="R6" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="5"/>
<contactref element="Y1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="6"/>
<contactref element="Y1" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP4" pad="D-"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="JP4" pad="D+"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="DP">
<contactref element="R5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="N$9">
<contactref element="JP4" pad="VBUS"/>
<contactref element="L1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="L1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C4" pad="A"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="DM">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="U1_BL_TX">
<contactref element="IC1" pad="30"/>
<contactref element="JP3" pad="7"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="U1_BL_RX">
<contactref element="IC1" pad="31"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="AIN1">
<contactref element="IC1" pad="10"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="T_JTDO">
<contactref element="R12" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="VD5" pad="C"/>
<contactref element="IC1" pad="16"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="43"/>
<contactref element="IC1" pad="46"/>
<contactref element="IC1" pad="21"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SWIM">
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="45"/>
<contactref element="R7" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="VD6" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="41"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="SWIM_RST">
<contactref element="IC1" pad="42"/>
<contactref element="R8" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="VD7" pad="C"/>
</signal>
<signal name="SWIM_H">
<contactref element="R17" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SWIM_RST_H">
<contactref element="R18" pad="1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="T_NRST">
<contactref element="R13" pad="2"/>
<contactref element="VD2" pad="C"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="T_NRST_H">
<contactref element="R13" pad="1"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="T_JRST">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="T_JTMS">
<contactref element="R14" pad="2"/>
<contactref element="VD3" pad="C"/>
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="T_JTMS_H">
<contactref element="R14" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="T_JTDI">
<contactref element="IC1" pad="17"/>
</signal>
<signal name="T_JTCK">
<contactref element="R15" pad="2"/>
<contactref element="VD4" pad="C"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="T_JTCK_H">
<contactref element="R15" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="T_JTDO_H">
<contactref element="R16" pad="1"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="25"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED2" pad="K"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="LED1" pad="A"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="MOUNTHOLE1">
</signal>
<signal name="MOUNTHOLE2">
</signal>
</signals>
</board>
</drawing>
</eagle>
