<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="53.175" x2="61.43" y2="53.175" width="0.4064" layer="20"/>
<wire x1="61.43" y1="53.175" x2="61.43" y2="0" width="0.4064" layer="20"/>
<wire x1="61.43" y1="0" x2="0" y2="0" width="0.4064" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="53.175" width="0.4064" layer="20"/>
<text>Global Hackathon Seoul
Intro to Arduino Shield</text>
<text>By Colin Szechy</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUEMILANOVE_VIAS">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ALPS_POT">
</package>
</packages>
</library>
<library name="MESH_Arduino">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Boards" package="DUEMILANOVE_VIAS" value="ARDUINO_SHIELDNO_SILK"/>
<element name="LED4" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED14" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="LED17" library="led" package="CHIPLED_0805" value=""/>
<element name="LED18" library="led" package="CHIPLED_0805" value=""/>
<element name="LED19" library="led" package="CHIPLED_0805" value=""/>
<element name="LED20" library="led" package="CHIPLED_0805" value=""/>
<element name="LED21" library="led" package="CHIPLED_0805" value=""/>
<element name="LED22" library="led" package="CHIPLED_0805" value=""/>
<element name="LED23" library="led" package="CHIPLED_0805" value=""/>
<element name="LED24" library="led" package="CHIPLED_0805" value=""/>
<element name="LED25" library="led" package="CHIPLED_0805" value=""/>
<element name="LED26" library="led" package="CHIPLED_0805" value=""/>
<element name="LED27" library="led" package="CHIPLED_0805" value=""/>
<element name="LED28" library="led" package="CHIPLED_0805" value=""/>
<element name="U$5" library="SparkFun-Electromechanical" package="ALPS_POT" value=""/>
<element name="S1" library="MESH_Arduino" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
</elements>
<signals>
<signal name="N$16">
<contactref element="U$1" pad="D2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="D3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="D4"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="D5"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="ROW1">
<contactref element="R1" pad="P$2"/>
<contactref element="LED22" pad="A"/>
<contactref element="LED21" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED28" pad="A"/>
</signal>
<signal name="ROW2">
<contactref element="R2" pad="P$2"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED14" pad="A"/>
</signal>
<signal name="ROW3">
<contactref element="R3" pad="P$2"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED23" pad="A"/>
</signal>
<signal name="ROW4">
<contactref element="R4" pad="P$2"/>
<contactref element="LED24" pad="A"/>
<contactref element="LED25" pad="A"/>
<contactref element="LED26" pad="A"/>
<contactref element="LED27" pad="A"/>
</signal>
<signal name="COL1">
<contactref element="U$1" pad="D7"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED28" pad="C"/>
<contactref element="LED23" pad="C"/>
<contactref element="LED27" pad="C"/>
</signal>
<signal name="COL2">
<contactref element="U$1" pad="D8"/>
<contactref element="LED9" pad="K"/>
<contactref element="LED22" pad="C"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED24" pad="C"/>
</signal>
<signal name="COL3">
<contactref element="U$1" pad="D9"/>
<contactref element="LED10" pad="K"/>
<contactref element="LED21" pad="C"/>
<contactref element="LED18" pad="C"/>
<contactref element="LED25" pad="C"/>
</signal>
<signal name="COL4">
<contactref element="U$1" pad="D10"/>
<contactref element="LED14" pad="K"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED26" pad="C"/>
</signal>
<signal name="GND">
<contactref element="U$5" pad="P$3"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="U$1" pad="GND@0"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="+5V">
<contactref element="U$5" pad="P$1"/>
<contactref element="U$1" pad="5V"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="POT">
<contactref element="U$1" pad="A0"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="BUTTON">
<contactref element="U$1" pad="D11"/>
<contactref element="R5" pad="P$1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
