<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.955" y2="0" width="0" layer="20"/>
<wire x1="20.955" y1="0" x2="20.955" y2="20.955" width="0" layer="20"/>
<wire x1="20.955" y1="20.955" x2="0" y2="20.955" width="0" layer="20"/>
<wire x1="0" y1="20.955" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>X+</text>
<text>Y+</text>
<text>X-</text>
<text>Y-</text>
<text>GND</text>
<text>VBAT</text>
<text>AUX</text>
<text>CLK</text>
<text>~CS</text>
<text>MOSI</text>
<text>BUSY</text>
<text>MISO</text>
<text>INT</text>
<text>IOVDD</text>
<text>VREF</text>
<text>VREF</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOP65P640X120-16N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Passives" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOP65P640X120-16N" value="TSC2046EQPWRQ1">
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="OC_NEWARK" value="84R0696"/>
<attribute name="MPN" value="TSC2046EQPWRQ1"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Passives" package="1X02" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="U1" pad="7"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="AUX">
<contactref element="U1" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="11"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="14"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="~CS">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="X+">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="Y+">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="X-">
<contactref element="U1" pad="4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="Y-">
<contactref element="U1" pad="5"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="12"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="BUSY">
<contactref element="U1" pad="13"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="IOVDD">
<contactref element="U1" pad="10"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
