<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="43.866" y2="0" width="0" layer="20"/>
<wire x1="43.866" y1="0" x2="43.866" y2="39.487" width="0" layer="20"/>
<wire x1="43.866" y1="39.487" x2="0" y2="39.487" width="0" layer="20"/>
<wire x1="0" y1="39.487" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.5146" y="29.972" drill="3.175"/>
<text>mBLE nRF51822</text>
<text>Main Board
Prototype V1</text>
<text>February 2015
Jason Leung</text>
<text>PWR
MAIN</text>
<text>PWR
DBUG</text>
<text>P0.29
P0.07</text>
<text>P0.28
P0.06</text>
<text>--------
P0.05</text>
<text>--------
P0.04</text>
<text>P0.25
P0.03</text>
<text>P0.24
P0.02</text>
<text>P0.23
P0.01</text>
<text>P0.22
P0.00</text>
<text>P0.30
P0.21
</text>
<text>+3V3 GND</text>
<text>--------
P0.08
</text>
<text>--------
P0.09
</text>
<text>--------
P0.10
</text>
<text>--------
P0.11
</text>
<text>--------
P0.12
</text>
<text>P0.17
P0.13
</text>
<text>P0.18
P0.14
</text>
<text>P0.19
P0.15
</text>
<text>P0.20
P0.16
</text>
<text>+3V3
GND
</text>
</plain>
<libraries>
<library name="mBLE">
<packages>
<package name="USB_MICRO_B-JST-MC5BR3-M404-4S-TB">
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
<package name="ANTENNA_U-FL">
</package>
<package name="OSC_3215">
</package>
<package name="CR2032_STRAP">
</package>
<package name="SOT23">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="M50-3600742">
</package>
<package name="1X06">
</package>
<package name="LED-0603">
</package>
<package name="SMALL-M-SOLDER">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="MAAV_13v1">
<description>Generated from &lt;b&gt;MAAV_Vehicle_13v1.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="RCL_R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="NordicSemi">
<packages>
<package name="QFN48">
</package>
<package name="2.5X2MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0402-CAP" value="12pF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0402-CAP" value="47nF">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0402-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="12pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402-CAP" value="2.2nF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0402-CAP" value="1.0pF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0402-CAP" value="2.2pF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0402-CAP" value="1.5pF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0402-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0402-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0402-CAP" value="1.0nF">
<attribute name="NAME"/>
</element>
<element name="J1" library="mBLE" package="USB_MICRO_B-JST-MC5BR3-M404-4S-TB" value="MICRO_USB">
<attribute name="MOUSER" value="53X3655"/>
<attribute name="DIGIKEY" value="455-2567-2-ND"/>
</element>
<element name="L1" library="SparkFun-Passives" package="C0402" value="4.7nH">
<attribute name="NAME"/>
</element>
<element name="L2" library="SparkFun-Passives" package="C0402" value="10nH"/>
<element name="L3" library="SparkFun-Passives" package="C0402" value="3.3nH">
<attribute name="NAME"/>
</element>
<element name="R3" library="MAAV_13v1" package="RCL_R0402" value="12k">
<attribute name="NAME"/>
</element>
<element name="U$1" library="NordicSemi" package="QFN48" value="NRF51822"/>
<element name="X2" library="NordicSemi" package="2.5X2MM" value="16MHz">
<attribute name="VALUE"/>
</element>
<element name="S1" library="mBLE" package="TACTILE-SWITCH-SMD" value="TAC_SWITCHSMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
</element>
<element name="S2" library="mBLE" package="TACTILE-SWITCH-SMD" value="TAC_SWITCHSMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
</element>
<element name="U$2" library="mBLE" package="ANTENNA_U-FL" value="ANTENNA-COAX">
<attribute name="HIROSE" value="U.FL-R-SMT-1(10)"/>
<attribute name="DIGIKEY" value="H11891CT-ND"/>
</element>
<element name="U$3" library="mBLE" package="OSC_3215" value="32kHz">
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0402-CAP" value="12pF">
<attribute name="NAME"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0402-CAP" value="12pF">
<attribute name="NAME"/>
</element>
<element name="U$4" library="mBLE" package="CR2032_STRAP" value="BATTERYSTRAP">
<attribute name="DIGIKEY" value="BC-2400-ND"/>
</element>
<element name="U$5" library="mBLE" package="SOT23" value="PMOSFET">
<attribute name="NAME"/>
</element>
<element name="U$6" library="mBLE" package="SOT23-5" value="LDO">
<attribute name="DIGIKEY" value="296-27893-1-ND"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0402-CAP" value="1uF cer">
<attribute name="NAME"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF cer">
<attribute name="NAME"/>
</element>
<element name="R1" library="MAAV_13v1" package="RCL_R0402" value="100k">
<attribute name="VALUE"/>
</element>
<element name="J2" library="mBLE" package="M50-3600742" value=""/>
<element name="J3" library="mBLE" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="SparkFun-Connectors" package="2X10" value="M10X2"/>
<element name="U$8" library="SparkFun-Connectors" package="2X10" value="M10X2"/>
<element name="PWR" library="mBLE" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
</element>
<element name="R2" library="MAAV_13v1" package="RCL_R0402" value="51">
<attribute name="NAME"/>
</element>
<element name="R4" library="MAAV_13v1" package="RCL_R0402" value="51">
<attribute name="NAME"/>
</element>
<element name="SWD" library="mBLE" package="LED-0603" value="AMBER">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS123LT1G">
<attribute name="PROD_ID" value="TRANS-08345"/>
<attribute name="NAME"/>
</element>
<element name="U$9" library="mBLE" package="SMALL-M-SOLDER" value=""/>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="U$1" pad="33"/>
<contactref element="U$1" pad="34"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="13"/>
<contactref element="C7" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="X2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="X2" pad="GND2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="GND@2"/>
<contactref element="U$2" pad="GND@1"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$4" pad="BAT-"/>
<contactref element="J2" pad="9"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$8" pad="20"/>
<contactref element="PWR" pad="C"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="C5" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="ANTENNA">
<contactref element="L3" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U$2" pad="SIG"/>
</signal>
<signal name="ANT2">
<contactref element="U$1" pad="32"/>
<contactref element="L1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="ANT1">
<contactref element="U$1" pad="31"/>
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="VDD_PA">
<contactref element="U$1" pad="30"/>
<contactref element="L2" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="XC2">
<contactref element="U$1" pad="38"/>
<contactref element="X2" pad="X1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="XC1">
<contactref element="U$1" pad="37"/>
<contactref element="X2" pad="X2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="DEC1">
<contactref element="U$1" pad="39"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="DEC2">
<contactref element="U$1" pad="29"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="U$1" pad="23"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="4"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="SWDCLK/NRESET">
<contactref element="U$1" pad="24"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="1"/>
<contactref element="U$6" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U$6" pad="5"/>
<contactref element="U$5" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U$1" pad="12"/>
<contactref element="C11" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U$1" pad="35"/>
<contactref element="U$1" pad="36"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$8" pad="19"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="P0.30">
<contactref element="U$1" pad="3"/>
<contactref element="U$7" pad="4"/>
</signal>
<signal name="P0.07">
<contactref element="U$1" pad="11"/>
<contactref element="U$7" pad="20"/>
</signal>
<signal name="XL1">
<contactref element="U$1" pad="46"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="XL2">
<contactref element="U$1" pad="45"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="+3V">
<contactref element="U$4" pad="BAT+@1"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="P0.00">
<contactref element="U$1" pad="4"/>
<contactref element="U$7" pad="6"/>
</signal>
<signal name="P0.01">
<contactref element="U$1" pad="5"/>
<contactref element="U$7" pad="8"/>
</signal>
<signal name="P0.02">
<contactref element="U$1" pad="6"/>
<contactref element="U$7" pad="10"/>
</signal>
<signal name="P0.03">
<contactref element="U$1" pad="7"/>
<contactref element="U$7" pad="12"/>
</signal>
<signal name="P0.04">
<contactref element="U$1" pad="8"/>
<contactref element="U$7" pad="14"/>
</signal>
<signal name="P0.05">
<contactref element="U$1" pad="9"/>
<contactref element="U$7" pad="16"/>
</signal>
<signal name="P0.06">
<contactref element="U$1" pad="10"/>
<contactref element="U$7" pad="18"/>
</signal>
<signal name="P0.29">
<contactref element="U$1" pad="48"/>
<contactref element="U$7" pad="19"/>
</signal>
<signal name="P0.28">
<contactref element="U$1" pad="47"/>
<contactref element="U$7" pad="17"/>
</signal>
<signal name="P0.25">
<contactref element="U$1" pad="44"/>
<contactref element="U$7" pad="11"/>
</signal>
<signal name="P0.24">
<contactref element="U$1" pad="43"/>
<contactref element="U$7" pad="9"/>
</signal>
<signal name="P0.23">
<contactref element="U$1" pad="42"/>
<contactref element="U$7" pad="7"/>
</signal>
<signal name="P0.22">
<contactref element="U$1" pad="41"/>
<contactref element="U$7" pad="5"/>
</signal>
<signal name="P0.21">
<contactref element="U$1" pad="40"/>
<contactref element="U$7" pad="3"/>
</signal>
<signal name="P0.20">
<contactref element="U$1" pad="28"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="U$8" pad="17"/>
</signal>
<signal name="P0.19">
<contactref element="U$1" pad="27"/>
<contactref element="U$8" pad="15"/>
</signal>
<signal name="P0.18">
<contactref element="U$1" pad="26"/>
<contactref element="U$8" pad="13"/>
</signal>
<signal name="P0.17">
<contactref element="U$1" pad="25"/>
<contactref element="U$8" pad="11"/>
</signal>
<signal name="P0.08">
<contactref element="U$1" pad="14"/>
<contactref element="U$8" pad="2"/>
</signal>
<signal name="P0.09">
<contactref element="U$1" pad="15"/>
<contactref element="U$8" pad="4"/>
</signal>
<signal name="P0.10">
<contactref element="U$1" pad="16"/>
<contactref element="U$8" pad="6"/>
</signal>
<signal name="P0.12">
<contactref element="U$1" pad="18"/>
<contactref element="U$8" pad="10"/>
</signal>
<signal name="P0.13">
<contactref element="U$1" pad="19"/>
<contactref element="U$8" pad="12"/>
</signal>
<signal name="P0.14">
<contactref element="U$1" pad="20"/>
<contactref element="U$8" pad="14"/>
</signal>
<signal name="P0.15">
<contactref element="U$1" pad="21"/>
<contactref element="U$8" pad="16"/>
</signal>
<signal name="P0.16">
<contactref element="U$1" pad="22"/>
<contactref element="U$8" pad="18"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$8" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U$8" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="U$8" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U$8" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="SWD" pad="C"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="SWD" pad="A"/>
</signal>
<signal name="P0.26">
<contactref element="U$7" pad="13"/>
</signal>
<signal name="P0.27">
<contactref element="U$7" pad="15"/>
</signal>
<signal name="P0.11">
<contactref element="U$1" pad="17"/>
<contactref element="U$8" pad="8"/>
</signal>
<signal name="+3V3A">
<contactref element="S3" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$6" pad="3"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="+3V3B">
<contactref element="S3" pad="3"/>
<contactref element="J3" pad="6"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
