<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="46.99" x2="13.97" y2="46.99" width="0" layer="20"/>
<wire x1="13.97" y1="46.99" x2="13.97" y2="80" width="0" layer="20"/>
<wire x1="13.97" y1="80" x2="-1.27" y2="80" width="0" layer="20"/>
<wire x1="-1.27" y1="80" x2="-1.27" y2="46.99" width="0" layer="20"/>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+TIP</text>
<text>2.1MM</text>
<text>+</text>
<text>-</text>
<text>TJP 5/2015</text>
<text>POWER
ADAPTOR</text>
<text>r2</text>
</plain>
<libraries>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCJ0202">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2.1MMDC" library="con-jack" package="DCJ0202" value="DCJ0202">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="JP2" library="pinhead" package="2X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="2.1MMDC" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="2.1MMDC" pad="1"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
