<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="43.18" y1="43.18" x2="0" y2="43.18" width="0" layer="20"/>
<wire x1="0" y1="43.18" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="43.18" y2="0" width="0" layer="20"/>
<text>BAT</text>
<text>G</text>
<text>BUS</text>
<text>5V</text>
<text>8</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>TX</text>
<text>RX</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>Ar</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>~</text>
<text>~</text>
<text>10</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>+</text>
<text>9</text>
<text>~</text>
<hole x="2.032" y="2.032" drill="3.2"/>
<hole x="2.032" y="41.148" drill="3.2"/>
<hole x="41.148" y="2.032" drill="3.2"/>
<hole x="41.148" y="41.148" drill="3.2"/>
<text>Y R Br</text>
<text>X</text>
<text>Y</text>
<text>Dial</text>
<wire x1="43.18" y1="0" x2="43.18" y2="43.18" width="0" layer="20"/>
<text>v1.1</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X12-CB">
</package>
<package name="JSTPH3">
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA7343">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP4" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="POT" library="adafruit" package="JSTPH3" value="">
<attribute name="VALUE"/>
</element>
<element name="POWER" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RUN_LED" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INT_LED" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SLP_LED" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X_SERVO" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="Y_SERVO" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LASER" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RUN_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/50V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="INT_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/50V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="SLEEP_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/50V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="LASER_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="200mA/50V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="X_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2.6A/20V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="Y_MOS" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2.6A/20V">
<attribute name="PROD_ID" value="TRANS-00830"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-11057"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-11057"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-11057"/>
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="39">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA7343" value="100uF">
<attribute name="PROD_ID" value="CAP-07890"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="POWER" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="POT" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="Y_SERVO" pad="3"/>
<contactref element="X_SERVO" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="LASER" pad="2"/>
<contactref element="C1" pad="C"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="JP1" pad="12"/>
</signal>
<signal name="D10">
<contactref element="JP4" pad="2"/>
</signal>
<signal name="D11">
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D12">
<contactref element="JP4" pad="4"/>
</signal>
<signal name="D13">
<contactref element="JP4" pad="5"/>
</signal>
<signal name="X_PWM_PIN">
<contactref element="JP4" pad="7"/>
<contactref element="X_SERVO" pad="3"/>
</signal>
<signal name="Y_PWM_PIN">
<contactref element="JP4" pad="8"/>
<contactref element="Y_SERVO" pad="1"/>
</signal>
<signal name="POT_IN">
<contactref element="JP4" pad="9"/>
<contactref element="POT" pad="2"/>
</signal>
<signal name="X_PWR_PIN">
<contactref element="JP4" pad="10"/>
<contactref element="X_MOS" pad="1"/>
</signal>
<signal name="Y_PWR_PIN">
<contactref element="JP4" pad="11"/>
<contactref element="Y_MOS" pad="1"/>
</signal>
<signal name="A5">
<contactref element="JP4" pad="12"/>
</signal>
<signal name="SLP_LED_PIN">
<contactref element="JP1" pad="9"/>
<contactref element="SLEEP_MOS" pad="1"/>
</signal>
<signal name="INT_LED_PIN">
<contactref element="JP1" pad="8"/>
<contactref element="INT_MOS" pad="1"/>
</signal>
<signal name="D6">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="D5">
<contactref element="JP1" pad="7"/>
</signal>
<signal name="TXD">
<contactref element="JP1" pad="10"/>
</signal>
<signal name="RXD">
<contactref element="JP1" pad="11"/>
</signal>
<signal name="RUN_LED_PIN">
<contactref element="JP1" pad="5"/>
<contactref element="RUN_MOS" pad="1"/>
</signal>
<signal name="LASER_PIN">
<contactref element="JP4" pad="1"/>
<contactref element="LASER_MOS" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="JP4" pad="6"/>
</signal>
<signal name="LASER_PWR">
<contactref element="LASER_MOS" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="X_MOS" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="X_SERVO" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Y_MOS" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="Y_SERVO" pad="2"/>
</signal>
<signal name="SLP_LED_PWR">
<contactref element="SLP_LED" pad="1"/>
<contactref element="SLEEP_MOS" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="INT_LED_PWR">
<contactref element="INT_LED" pad="1"/>
<contactref element="INT_MOS" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RUN_LED_PWR">
<contactref element="RUN_LED" pad="1"/>
<contactref element="RUN_MOS" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="RUN_LED" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="SLP_LED" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="2"/>
<contactref element="INT_LED" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R10" pad="1"/>
<contactref element="LASER" pad="1"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="4"/>
<contactref element="POT" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="JP1" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="LASER_MOS" pad="3"/>
<contactref element="X_MOS" pad="3"/>
<contactref element="Y_MOS" pad="3"/>
<contactref element="SLEEP_MOS" pad="3"/>
<contactref element="INT_MOS" pad="3"/>
<contactref element="RUN_MOS" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
