<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="175" y2="0" width="0" layer="20"/>
<wire x1="175" y1="0" x2="175" y2="45" width="0" layer="20"/>
<wire x1="175" y1="45" x2="0" y2="45" width="0" layer="20"/>
<wire x1="0" y1="45" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="TRIM_POT_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="1206">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DPAK">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="FTDI_DEVICE_SIDE">
<description>Package for devices meant to mate to an FTDI connector.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="UP" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="DOWN" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="SELECT" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="CH1" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="CH2" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="CH3" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="CH4" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="CH5" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="CH6" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="R1" library="SparkFun-Passives" package="1206" value="3K3"/>
<element name="R2" library="SparkFun-Passives" package="1206" value="1K"/>
<element name="R3" library="SparkFun-Passives" package="1206" value="620R"/>
<element name="R4" library="SparkFun-Passives" package="1206" value="330R"/>
<element name="R5" library="SparkFun-Passives" package="1206" value="2K"/>
<element name="-/+" library="SparkFun-Passives" package="1X02" value="BATTERY"/>
<element name="R6" library="SparkFun-Electromechanical" package="TRIM_POT_PTH" value="TRIMPOTPTH"/>
<element name="RF-MODULE" library="SparkFun-Passives" package="1X03" value="JUMPER-3PTH"/>
<element name="ROT.SWITCH" library="SparkFun-Passives" package="1X03" value="LEFT-RIGHT"/>
<element name="U$1" library="SparkFun-PowerIC" package="DPAK" value="7805"/>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value=""/>
<element name="R7" library="SparkFun-Passives" package="1206" value="330R"/>
<element name="R8" library="SparkFun-Passives" package="1206" value="2K"/>
<element name="R9" library="SparkFun-Passives" package="1206" value="2K"/>
<element name="DR" library="SparkFun-Passives" package="1X02" value=""/>
<element name="TC" library="SparkFun-Passives" package="1X02" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="FTDI_DEVICE_SIDE" value="FTDI_DEVICE"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="U$1" pad="4"/>
<contactref element="-/+" pad="2"/>
<contactref element="RF-MODULE" pad="1"/>
<contactref element="CH1" pad="1"/>
<contactref element="CH2" pad="1"/>
<contactref element="CH3" pad="1"/>
<contactref element="CH4" pad="1"/>
<contactref element="CH5" pad="1"/>
<contactref element="CH6" pad="1"/>
<contactref element="R6" pad="3"/>
<contactref element="DR" pad="2"/>
<contactref element="TC" pad="2"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP2" pad="P$6"/>
<contactref element="UP" pad="4"/>
<contactref element="DOWN" pad="4"/>
<contactref element="SELECT" pad="4"/>
<contactref element="ROT.SWITCH" pad="2"/>
</signal>
<signal name="V_BATT">
<contactref element="U$1" pad="1"/>
<contactref element="-/+" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="24"/>
<contactref element="CH1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="25"/>
<contactref element="CH2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="27"/>
<contactref element="CH4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="28"/>
<contactref element="CH5" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="19"/>
<contactref element="CH6" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="SELECT" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="ROT.SWITCH" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="1"/>
<contactref element="DOWN" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="UP" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="23"/>
<contactref element="ROT.SWITCH" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="11"/>
<contactref element="RF-MODULE" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="26"/>
<contactref element="CH3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="CH6" pad="2"/>
<contactref element="CH5" pad="2"/>
<contactref element="CH4" pad="2"/>
<contactref element="CH3" pad="2"/>
<contactref element="RF-MODULE" pad="2"/>
<contactref element="CH1" pad="2"/>
<contactref element="CH2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="P$4"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="31"/>
<contactref element="DR" pad="1"/>
<contactref element="JP2" pad="P$3"/>
</signal>
<signal name="N$22">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="TC" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="JP1" pad="7"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$18">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$20">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$21">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$23">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="30"/>
<contactref element="JP2" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
