<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="8.105140625" width="0" layer="20"/>
<wire x1="0" y1="8.105140625" x2="11.389359375" y2="8.105140625" width="0" layer="20"/>
<wire x1="11.389359375" y1="8.105140625" x2="11.389359375" y2="0" width="0" layer="20"/>
<wire x1="11.389359375" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>PSON</text>
<text>POK</text>
</plain>
<libraries>
<library name="headers(2mm)">
<packages>
<package name="2X5">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JIN" library="headers(2mm)" package="2X5" value="2X5"/>
<element name="JOUT" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="1,6/0,9" value="WIREPAD1,6/0,9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JIN" pad="2"/>
<contactref element="JIN" pad="10"/>
<contactref element="JIN" pad="1"/>
<contactref element="JOUT" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="JIN" pad="3"/>
</signal>
<signal name="PSON">
<contactref element="JIN" pad="4"/>
<contactref element="JIN" pad="5"/>
<contactref element="JOUT" pad="1"/>
</signal>
<signal name="POK">
<contactref element="JIN" pad="7"/>
<contactref element="JOUT" pad="3"/>
</signal>
<signal name="VS+">
<contactref element="JIN" pad="6"/>
</signal>
<signal name="VS-">
<contactref element="JIN" pad="8"/>
</signal>
<signal name="IS">
<contactref element="JIN" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
