<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="17.78" x2="20.32" y2="17.78" width="0" layer="20"/>
<wire x1="20.32" y1="17.78" x2="71.1075" y2="17.78" width="0" layer="20"/>
<wire x1="71.1075" y1="17.78" x2="71.1075" y2="76.19" width="0" layer="20"/>
<wire x1="71.1075" y1="76.19" x2="17.78" y2="76.19" width="0" layer="20"/>
<wire x1="17.78" y1="76.19" x2="17.78" y2="20.32" width="0" layer="20"/>
<text>CageLogger V1.0
(C) F. Hage 2015</text>
<wire x1="17.78" y1="20.32" x2="17.78" y2="17.78" width="0" layer="20"/>
<wire x1="17.78" y1="20.32" x2="17.78" y2="73.66" width="0.4064" layer="20"/>
<wire x1="17.78" y1="73.66" x2="20.32" y2="76.2" width="0.4064" layer="20"/>
<wire x1="20.32" y1="76.2" x2="68.58" y2="76.2" width="0.4064" layer="20"/>
<wire x1="68.58" y1="76.2" x2="71.12" y2="73.66" width="0.4064" layer="20"/>
<wire x1="71.12" y1="73.66" x2="71.12" y2="20.32" width="0.4064" layer="20"/>
<wire x1="71.12" y1="20.32" x2="68.58" y2="17.78" width="0.4064" layer="20"/>
<wire x1="68.58" y1="17.78" x2="20.32" y2="17.78" width="0.4064" layer="20"/>
<wire x1="20.32" y1="17.78" x2="17.78" y2="20.32" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ11-6">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JA" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
</element>
<element name="JB" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
</element>
<element name="JC" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
</element>
<element name="JD" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
</element>
<element name="JE" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
</element>
<element name="SW1" library="special" package="EDG-04" value="Group Sel">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="D5"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="D6"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="D7"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="D8"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="D9"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="P$2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="P$2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="P$2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="P$2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="P$2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="GND@0"/>
<contactref element="D5" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="D2" pad="K"/>
<contactref element="D1" pad="K"/>
<contactref element="J1" pad="GND@1"/>
<contactref element="J1" pad="GND@2"/>
<contactref element="JB" pad="2"/>
<contactref element="JC" pad="2"/>
<contactref element="JD" pad="2"/>
<contactref element="JE" pad="2"/>
<contactref element="SW1" pad="8"/>
<contactref element="SW1" pad="7"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="5"/>
<contactref element="JA" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R10" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="R6" pad="P$1"/>
<contactref element="J1" pad="5V"/>
<contactref element="JA" pad="5"/>
<contactref element="JD" pad="5"/>
<contactref element="JE" pad="5"/>
<contactref element="JB" pad="5"/>
<contactref element="JC" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="R8" pad="P$2"/>
<contactref element="JC" pad="4"/>
<contactref element="J1" pad="D2"/>
</signal>
<signal name="N$20">
<contactref element="R7" pad="P$2"/>
<contactref element="J1" pad="D3"/>
<contactref element="JD" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="R6" pad="P$2"/>
<contactref element="J1" pad="D4"/>
<contactref element="JE" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="D10"/>
<contactref element="R10" pad="P$2"/>
<contactref element="JA" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="R9" pad="P$2"/>
<contactref element="J1" pad="A4"/>
<contactref element="JB" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="SW1" pad="1"/>
<contactref element="J1" pad="A0"/>
</signal>
<signal name="N$15">
<contactref element="SW1" pad="2"/>
<contactref element="J1" pad="A1"/>
</signal>
<signal name="N$17">
<contactref element="SW1" pad="3"/>
<contactref element="J1" pad="A2"/>
</signal>
<signal name="N$18">
<contactref element="SW1" pad="4"/>
<contactref element="J1" pad="A3"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
