<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="10.16" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="6.567896875" y2="0" width="0" layer="20"/>
<wire x1="6.567896875" y1="0" x2="8.36395" y2="0.74395" width="0" layer="20" curve="45.00005"/>
<wire x1="8.36395" y1="0.74395" x2="9.41605" y2="1.79605" width="0" layer="20"/>
<wire x1="9.41605" y1="1.79605" x2="11.212103125" y2="2.54" width="0" layer="20" curve="-45.00007"/>
<wire x1="11.212103125" y1="2.54" x2="15.24" y2="2.54" width="0" layer="20"/>
<wire x1="15.24" y1="2.54" x2="17.78" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="5.08" x2="17.78" y2="7.62" width="0" layer="20"/>
<wire x1="17.78" y1="7.62" x2="15.24" y2="10.16" width="0" layer="20" curve="90"/>
<wire x1="15.24" y1="10.16" x2="11.212103125" y2="10.16" width="0" layer="20"/>
<wire x1="11.212103125" y1="10.16" x2="9.41605" y2="10.90395" width="0" layer="20" curve="-45.00005"/>
<wire x1="9.41605" y1="10.90395" x2="8.36395" y2="11.95605" width="0" layer="20"/>
<wire x1="8.36395" y1="11.95605" x2="6.567896875" y2="12.7" width="0" layer="20" curve="45.00007"/>
<wire x1="6.567896875" y1="12.7" x2="2.54" y2="12.7" width="0" layer="20"/>
<wire x1="2.54" y1="12.7" x2="0" y2="10.16" width="0" layer="20" curve="90"/>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>Barbary</text>
<text>Enterprises</text>
<text>USB MiniB</text>
<text>Power</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="USB-MINIB-THM-MOLEX-PWRONLY">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="adafruit" package="USB-MINIB-THM-MOLEX-PWRONLY" value="USB-PWR"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="VBUS"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
