<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="12.7" width="0" layer="20"/>
<wire x1="50" y1="12.7" x2="0" y2="12.7" width="0" layer="20"/>
<hole x="2.2225" y="10.4775" drill="2"/>
<hole x="2.2225" y="2.2225" drill="2"/>
<text>2013</text>
<text>pfriedel</text>
<text>\\O_o/</text>
<text>v4</text>
<text>3-4.5v</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>ATtiny85</text>
<text>Stick Ed!</text>
<text>v4: Refactored to pass OSH DRC.</text>
<text>-</text>
<text>+</text>
<text>C1</text>
<text>R6</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="LED-TRICOLOR-5050">
<description>&lt;H3&gt;5050 SMD RGB LED&lt;/h3&gt;
5.0mm x 5.0mm, 2.6mm thickness</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="00_PERSONAL">
<packages>
<package name="6X3MM-TACT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="+" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="-" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun" package="SO08-EIAJ" value="ATTINY85"/>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
<element name="MODE" library="00_PERSONAL" package="6X3MM-TACT" value="3X6MM_SWITCH"/>
<element name="LED3" library="SparkFun" package="LED-TRICOLOR-5050" value="LED-TRICOLOR-5050"/>
<element name="LED4" library="SparkFun" package="LED-TRICOLOR-5050" value="LED-TRICOLOR-5050"/>
<element name="LED5" library="SparkFun" package="LED-TRICOLOR-5050" value="LED-TRICOLOR-5050"/>
<element name="LED1" library="SparkFun" package="LED-TRICOLOR-5050" value="LED-TRICOLOR-5050"/>
<element name="LED2" library="SparkFun" package="LED-TRICOLOR-5050" value="LED-TRICOLOR-5050"/>
<element name="C1" library="adafruit" package="C0805K" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RST">
<contactref element="R6" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="MODE" pad="P$1"/>
</signal>
<signal name="2R">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="3R">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="-" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="MODE" pad="P$2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="+" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="7R">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="6R">
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5R">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
<signal name="E">
<contactref element="LED3" pad="6"/>
<contactref element="LED5" pad="5"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED1" pad="3"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="D">
<contactref element="LED3" pad="4"/>
<contactref element="LED4" pad="6"/>
<contactref element="LED1" pad="5"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="B">
<contactref element="LED3" pad="5"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED4" pad="3"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED5" pad="4"/>
<contactref element="LED1" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="C">
<contactref element="LED3" pad="1"/>
<contactref element="LED3" pad="3"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED5" pad="6"/>
<contactref element="LED2" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="A">
<contactref element="LED4" pad="5"/>
<contactref element="LED5" pad="1"/>
<contactref element="LED5" pad="3"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED1" pad="4"/>
<contactref element="LED2" pad="6"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
