<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.81" y2="0" width="0" layer="20"/>
<wire x1="36.81" y1="0" x2="36.81" y2="28.88" width="0" layer="20"/>
<wire x1="36.81" y1="28.88" x2="0" y2="28.88" width="0" layer="20"/>
<wire x1="0" y1="28.88" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-5MM">
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="avr-7" package="AVR-ISP-6" value="AVR-ISP-6VERT"/>
<element name="U$1" library="avr-7" package="DIL20" value="TINY2313-*P*"/>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49U-V" value=""/>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-5MM" value=""/>
<element name="C2" library="SparkFun-Passives" package="CAP-PTH-5MM" value=""/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.5" value=""/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-3_LOCK.007S" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="10"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="18"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="17"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="19"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="4"/>
<contactref element="Y1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="5"/>
<contactref element="Y1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="20"/>
<contactref element="JP1" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J1" pad="PWR"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="12"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
