<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="2.286" y1="25.146" x2="40.386" y2="25.146" width="0.4064" layer="20"/>
<wire x1="40.386" y1="25.146" x2="40.386" y2="2.286" width="0.4064" layer="20"/>
<wire x1="40.386" y1="2.286" x2="2.286" y2="2.286" width="0.4064" layer="20"/>
<wire x1="2.286" y1="2.286" x2="2.286" y2="25.146" width="0.4064" layer="20"/>
<text>Linkit connect w Arduino</text>
</plain>
<libraries>
<library name="template">
<packages>
<package name="31P-L18.0XW15.0MM">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603-RES">
</package>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="QFN-44-NOPAD_1:1-OUTFAKES">
</package>
<package name="USB-AB-MICRO-SMD-V03-IN&amp;OUT">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="template" package="31P-L18.0XW15.0MM" value="MT7681_MOD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun" package="LED-0603" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="Testing" package="QFN-44-NOPAD_1:1-OUTFAKES" value="ATMEGA32U4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun" package="LED-0603" value="Yellow">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0603-RES" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0603-RES" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="Testing" package="USB-AB-MICRO-SMD-V03-IN&amp;OUT" value=""/>
<element name="Y2" library="SparkFun-FreqCtrl" package="RESONATOR-SMD" value="8MHZ">
<attribute name="PROD_ID" value="XTAL-08895"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="V_REG_LDOSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value=""/>
<element name="C1" library="SparkFun" package="0805" value="1uF"/>
<element name="C2" library="SparkFun" package="0805" value="1uF"/>
<element name="C3" library="SparkFun" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X15_LOCK" value="M15LOCK">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X15_LOCK" value="M15LOCK">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="15"/>
<contactref element="U3" pad="43"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="23"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="33"/>
<contactref element="C11" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="X1" pad="GND1"/>
<contactref element="Y2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="12"/>
<contactref element="JP1" pad="13"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="42"/>
</signal>
<signal name="RESET">
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="13"/>
<contactref element="U1" pad="8"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U3" pad="9"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="U3" pad="11"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="MOSI">
<contactref element="U3" pad="10"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="TXO">
<contactref element="U3" pad="21"/>
<contactref element="U1" pad="10"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="VCC">
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="14"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="24"/>
<contactref element="U3" pad="44"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D9">
<contactref element="U3" pad="29"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D8">
<contactref element="U3" pad="28"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="A5">
<contactref element="U3" pad="41"/>
</signal>
<signal name="A4">
<contactref element="U3" pad="40"/>
</signal>
<signal name="A3">
<contactref element="U3" pad="39"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="A2">
<contactref element="U3" pad="38"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="A1">
<contactref element="U3" pad="37"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="A0">
<contactref element="U3" pad="36"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="D2">
<contactref element="U3" pad="19"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="D3">
<contactref element="U3" pad="18"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="D4">
<contactref element="U3" pad="25"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D5">
<contactref element="U3" pad="31"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="D6">
<contactref element="U3" pad="27"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="D7">
<contactref element="U3" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="D10">
<contactref element="U3" pad="30"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="RXI">
<contactref element="U3" pad="20"/>
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="N$12">
<contactref element="U3" pad="6"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="UVCC">
<contactref element="U3" pad="7"/>
<contactref element="C14" pad="2"/>
<contactref element="X1" pad="VBUS1"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="D-">
<contactref element="U3" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D+">
<contactref element="U3" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="D11">
<contactref element="U3" pad="12"/>
</signal>
<signal name="D12">
<contactref element="U3" pad="26"/>
</signal>
<signal name="D13">
<contactref element="U3" pad="32"/>
</signal>
<signal name="D14">
<contactref element="U3" pad="8"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="TXLED">
<contactref element="U3" pad="22"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="2"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="R11" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="X1" pad="D-1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="X1" pad="D+1"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="16"/>
<contactref element="Y2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U3" pad="17"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="RAW">
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="13"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="14"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="15"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
