<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-1.035" y1="-0.935" x2="14.985" y2="-0.935" width="0" layer="20"/>
<wire x1="14.985" y1="-0.935" x2="14.985" y2="8.86" width="0" layer="20"/>
<wire x1="14.985" y1="8.86" x2="-1.035" y2="8.86" width="0" layer="20"/>
<wire x1="-1.035" y1="8.86" x2="-1.035" y2="-0.935" width="0" layer="20"/>
<text>!CS</text>
<text>SCLK</text>
<text>SDATA</text>
<text>VIN</text>
<text>GND</text>
<text>3.3V</text>
<text>AD7276 Breakout
Clemson University
Josiah Hester</text>
</plain>
<libraries>
<library name="adc">
<packages>
<package name="TSOT23-6">
<description>&lt;b&gt;S6 Package 6-Lead Plastic TSOT-23&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="adc" package="TSOT23-6" value="AD7276"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="!CS">
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SDATA">
<contactref element="U1" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
