<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="77.45" y2="0" width="0" layer="20"/>
<wire x1="77.45" y1="0" x2="77.45" y2="35.865" width="0" layer="20"/>
<wire x1="77.45" y1="35.865" x2="0" y2="35.865" width="0" layer="20"/>
<wire x1="0" y1="35.865" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="PIC18F46K80">
<packages>
<package name="PDIP40_600MC">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Pickit3">
<packages>
<package name="PICKIT3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X2-3.5MM">
</package>
</packages>
</library>
<library name="Bluetooth">
<packages>
<package name="1X04-BIG">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="1X11">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="PIC18F46K80" package="PDIP40_600MC" value="PIC18F46K22-X_P"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1nF"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1nF"/>
<element name="U$6" library="Pickit3" package="PICKIT3" value=""/>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="U$7" library="Bluetooth" package="1X04-BIG" value="BLUETOOTH"/>
<element name="U3" library="SparkFun" package="SO08" value="MCP2551"/>
<element name="IC1" library="74xx-eu" package="DIL14" value="7432N"/>
<element name="J2" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="JP3" library="SparkFun" package="1X11" value="MPU-9150"/>
<element name="JP1" library="pinhead" package="2X16" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="7"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP3" pad="11"/>
<contactref element="JP1" pad="30"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="14"/>
<contactref element="JP1" pad="22"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="14"/>
<contactref element="U3" pad="3"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="U1" pad="32"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="10"/>
<contactref element="JP1" pad="32"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP1" pad="16"/>
<contactref element="JP1" pad="24"/>
</signal>
<signal name="AD1-H">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="AD2-H">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="AD3-H">
<contactref element="U1" pad="10"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="N$23">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="MCLR">
<contactref element="U$6" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="PGD">
<contactref element="U$6" pad="P$4"/>
<contactref element="U1" pad="40"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="PGC">
<contactref element="U$6" pad="P$5"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="TXD">
<contactref element="U$7" pad="3"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="RXD">
<contactref element="U$7" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="CANL">
<contactref element="U3" pad="6"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="CANH">
<contactref element="U3" pad="7"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="CANTX">
<contactref element="U3" pad="1"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="CANRX">
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="DEMUX1-H">
<contactref element="U1" pad="22"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DEMUX2-H">
<contactref element="U1" pad="27"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="DEMUX3-H">
<contactref element="U1" pad="28"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="DEMUX4-H">
<contactref element="U1" pad="29"/>
<contactref element="JP1" pad="26"/>
</signal>
<signal name="AD4-H">
<contactref element="U1" pad="19"/>
<contactref element="JP1" pad="19"/>
<contactref element="JP1" pad="27"/>
</signal>
<signal name="AD5-H">
<contactref element="U1" pad="20"/>
<contactref element="JP1" pad="21"/>
<contactref element="JP1" pad="29"/>
</signal>
<signal name="AD6-H">
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="23"/>
<contactref element="JP1" pad="31"/>
</signal>
<signal name="ORGATE1">
<contactref element="U1" pad="17"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="18"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="23"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="33"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MUX1-H">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MUX2-H">
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="MUX3-H">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="MUX4-H">
<contactref element="IC1" pad="5"/>
<contactref element="JP1" pad="28"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
