<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="37.77" y2="0" width="0" layer="20"/>
<wire x1="37.77" y1="0" x2="37.77" y2="76.19" width="0" layer="20"/>
<wire x1="37.77" y1="76.19" x2="0" y2="76.19" width="0" layer="20"/>
<wire x1="0" y1="76.19" x2="0" y2="0" width="0" layer="20"/>
<text>ProMicroButtonBar
v1.2</text>
<text>06-12-2013</text>
<text>VCC</text>
<text>ProMicro</text>
<text>SparkFun</text>
<text>RDMJr.</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.5" value="100Ω"/>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R12" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R13" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R14" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R15" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R16" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R17" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R18" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R19" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="R20" library="SparkFun-Resistors" package="AXIAL-0.5" value="10KΩ"/>
<element name="JP3" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP4" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="R1" pad="P$1"/>
<contactref element="R11" pad="P$2"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="R12" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="R13" pad="P$2"/>
<contactref element="R3" pad="P$1"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R14" pad="P$2"/>
<contactref element="R4" pad="P$1"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="R15" pad="P$2"/>
<contactref element="R5" pad="P$1"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R16" pad="P$2"/>
<contactref element="R6" pad="P$1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="R17" pad="P$2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R18" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R19" pad="P$2"/>
<contactref element="R9" pad="P$1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R20" pad="P$2"/>
<contactref element="R10" pad="P$1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R11" pad="P$1"/>
<contactref element="R12" pad="P$1"/>
<contactref element="R13" pad="P$1"/>
<contactref element="R14" pad="P$1"/>
<contactref element="R15" pad="P$1"/>
<contactref element="R16" pad="P$1"/>
<contactref element="R17" pad="P$1"/>
<contactref element="R18" pad="P$1"/>
<contactref element="R19" pad="P$1"/>
<contactref element="R20" pad="P$1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="JP4" pad="10"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP4" pad="8"/>
<contactref element="JP4" pad="9"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="5"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="6"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="7"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="8"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="9"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="10"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="11"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="12"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="13"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="14"/>
<contactref element="R10" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
