<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="3.81" x2="1.27" y2="57.15" width="0.2032" layer="20"/>
<wire x1="1.27" y1="57.15" x2="2.54" y2="58.42" width="0.2032" layer="20"/>
<wire x1="2.54" y1="58.42" x2="13.97" y2="58.42" width="0.2032" layer="20"/>
<wire x1="13.97" y1="58.42" x2="16.51" y2="60.96" width="0.2032" layer="20"/>
<wire x1="16.51" y1="60.96" x2="49.53" y2="60.96" width="0.2032" layer="20"/>
<wire x1="49.53" y1="60.96" x2="52.07" y2="58.42" width="0.2032" layer="20"/>
<wire x1="52.07" y1="58.42" x2="54.61" y2="58.42" width="0.2032" layer="20"/>
<wire x1="54.61" y1="58.42" x2="54.61" y2="3.81" width="0.2032" layer="20"/>
<wire x1="54.61" y1="3.81" x2="52.07" y2="1.27" width="0.2032" layer="20"/>
<wire x1="52.07" y1="1.27" x2="3.81" y2="1.27" width="0.2032" layer="20"/>
<wire x1="3.81" y1="1.27" x2="1.27" y2="3.81" width="0.2032" layer="20"/>
<text>JP1
Closed</text>
<text>JP2
Open</text>
<text>JP3
Relay</text>
<text>Q1</text>
<text>R1</text>
<text>R2</text>
<text>D1</text>
<text>  2014 EmptyJay
Garage Door
Monitor</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4001-KIT">
</package>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-3-PTH">
</package>
<package name="JST-2-PTH">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="EmptyJay">
<packages>
<package name="RELAY-G5V">
<description>Radio Shack SPDT Relay 275-0241</description>
</package>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001-KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="JST-3-PTH" value="">
<attribute name="SKU" value="PRT-09915"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="JST-3-PTH" value="">
<attribute name="SKU" value="PRT-09915"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2">
<attribute name="SKU" value="PRT-09914"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="24K"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="10K"/>
<element name="U$2" library="EmptyJay" package="RELAY-G5V" value="RELAY-2G5Q"/>
<element name="U$3" library="EmptyJay" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
</elements>
<signals>
<signal name="VIN">
<contactref element="D1" pad="C"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$3" pad="VIN"/>
</signal>
<signal name="5V">
<contactref element="U$3" pad="5V"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$3" pad="GND@1"/>
<contactref element="Q1" pad="3"/>
<contactref element="U$3" pad="GND@2"/>
<contactref element="U$3" pad="GND@0"/>
<contactref element="R2" pad="P$1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="D4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="D5"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="P$2"/>
<contactref element="U$3" pad="D6"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="A"/>
<contactref element="Q1" pad="1"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="6"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
