<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>EVG2000 - 1/4/14 - INTV Vid Mod V1</text>
<wire x1="4.699" y1="26.162" x2="29.718" y2="26.162" width="0.3048" layer="20"/>
<wire x1="29.718" y1="26.162" x2="29.718" y2="1.27" width="0.3048" layer="20"/>
<wire x1="29.718" y1="1.27" x2="4.699" y2="1.27" width="0.3048" layer="20"/>
<wire x1="4.699" y1="1.27" x2="4.699" y2="26.162" width="0.3048" layer="20"/>
</plain>
<libraries>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP10">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AI" library="solpad" package="LSP10" value="LSP10"/>
<element name="AO" library="solpad" package="LSP10" value="LSP10"/>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="GND" library="solpad" package="LSP10" value="LSP10"/>
<element name="V-IN" library="solpad" package="LSP10" value="LSP10"/>
<element name="VO" library="solpad" package="LSP10" value="LSP10"/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="2n3904"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="2n3904"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="51k"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="33k"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="660"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.1" value="330"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="15k"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.1" value="22k"/>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.1" value="75"/>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.1" value="22"/>
<element name="+5V" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VG" library="solpad" package="LSP10" value="LSP10"/>
<element name="AG" library="solpad" package="LSP10" value="LSP10"/>
</elements>
<signals>
<signal name="GNDX">
<contactref element="R6" pad="P$2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="GND" pad="MP"/>
<contactref element="VG" pad="MP"/>
<contactref element="AG" pad="MP"/>
</signal>
<signal name="N$3">
<contactref element="VO" pad="MP"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="P$1"/>
<contactref element="Q1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C2" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="P$1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="V-IN" pad="MP"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="P$1"/>
<contactref element="Q2" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="+5V" pad="MP"/>
</signal>
<signal name="N$1">
<contactref element="C4" pad="1"/>
<contactref element="AI" pad="MP"/>
</signal>
<signal name="N$2">
<contactref element="AO" pad="MP"/>
<contactref element="C4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
