<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.0508" y1="-0.0508" x2="15.2908" y2="-0.0508" width="0" layer="20"/>
<wire x1="15.2908" y1="-0.0508" x2="15.2908" y2="12.7" width="0" layer="20"/>
<wire x1="15.2908" y1="12.7" x2="15.2908" y2="19.9898" width="0" layer="20"/>
<wire x1="15.2908" y1="19.9898" x2="7.62" y2="19.9898" width="0" layer="20"/>
<text>.1u</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>3.3V</text>
<text>SCL</text>
<text>SCL</text>
<text>SDA</text>
<text>SDA</text>
<hole x="7.62" y="15.24" drill="5.08"/>
<wire x1="7.62" y1="19.9898" x2="-0.0508" y2="19.9898" width="0" layer="20"/>
<wire x1="-0.0508" y1="19.9898" x2="-0.0508" y2="12.7" width="0" layer="20"/>
<wire x1="-0.0508" y1="12.7" x2="-0.0508" y2="-0.0508" width="0" layer="20"/>
<wire x1="-0.0508" y1="12.7" x2="7.62" y2="19.9898" width="0" layer="20" curve="-90"/>
<wire x1="7.62" y1="19.9898" x2="15.2908" y2="12.7" width="0" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="Eds Library">
<packages>
<package name="MLX90614XXX">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Eds Library" package="MLX90614XXX" value="MLX90614"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="SDA">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="VDD">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
