<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="1.27" x2="19.99" y2="1.27" width="0" layer="20"/>
<wire x1="19.99" y1="1.27" x2="19.99" y2="24.12" width="0" layer="20"/>
<wire x1="19.99" y1="24.12" x2="2.54" y2="24.12" width="0" layer="20"/>
<wire x1="2.54" y1="24.12" x2="2.54" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="8"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="7"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
