<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="72.06" y2="0" width="0" layer="20"/>
<wire x1="72.06" y1="0" x2="72.06" y2="38.09" width="0" layer="20"/>
<wire x1="72.06" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="34.29" drill="3.2639"/>
<hole x="3.81" y="3.81" drill="3.2639"/>
<hole x="68.58" y="3.81" drill="3.2639"/>
<hole x="68.58" y="34.29" drill="3.2639"/>
<text>CyberAntics 2015
Ramon Yvarra</text>
<text>Input</text>
<text>Ouput</text>
<text>Mouse Piano
Solenoid Board V2</text>
<text>Amelia's dance was quick and magical
as each tiny paw fluttered across
the keys.</text>
</plain>
<libraries>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="DIP254P762X508-20">
</package>
</packages>
</library>
<library name="con-phoenix-254">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 2.54 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FFKDS">
</package>
<package name="FFKDS-END">
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FFKV2">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="DIP254P762X508-20" value="TPIC6A596NE">
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="OC_NEWARK" value="55M8243"/>
<attribute name="MPN" value="TPIC6B259N"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="2+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="2-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="3+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="3-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="4+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="4-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="1+" library="con-phoenix-254" package="FFKDS-END" value="Solenoid Inputs">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="5-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="6+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="6-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="7+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="7-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="8+" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="8-" library="con-phoenix-254" package="FFKDS" value="FFKDS"/>
<element name="JP2" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="12V" library="con-phoenix-508" package="FFKV2" value="FFKV2">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="17"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="19"/>
<contactref element="1-" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="20"/>
<contactref element="2-" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="3-" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="2"/>
<contactref element="4-" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="9"/>
<contactref element="5-" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="10"/>
<contactref element="6-" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="11"/>
<contactref element="7-" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="12"/>
<contactref element="8-" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="8+" pad="P$1"/>
<contactref element="7+" pad="P$1"/>
<contactref element="6+" pad="P$1"/>
<contactref element="5+" pad="P$1"/>
<contactref element="4+" pad="P$1"/>
<contactref element="3+" pad="P$1"/>
<contactref element="2+" pad="P$1"/>
<contactref element="1+" pad="P$1"/>
<contactref element="12V" pad="1"/>
<contactref element="12V" pad="1A"/>
</signal>
<signal name="PGND">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="15"/>
<contactref element="12V" pad="2"/>
<contactref element="12V" pad="2A"/>
</signal>
<signal name="RCK">
<contactref element="JP2" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SRCK">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="LGND">
<contactref element="JP2" pad="6"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SRCLR">
<contactref element="JP2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SEROUT">
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="SERIN">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
