<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="25.654" y1="43.18" x2="25.654" y2="-0.254" width="0.2032" layer="20"/>
<wire x1="25.654" y1="-0.254" x2="-0.254" y2="-0.254" width="0.2032" layer="20"/>
<wire x1="-0.254" y1="-0.254" x2="-0.254" y2="43.18" width="0.2032" layer="20"/>
<wire x1="25.654" y1="43.18" x2="26.67" y2="44.45" width="0.2032" layer="20"/>
<wire x1="26.67" y1="44.45" x2="26.67" y2="64.77" width="0.2032" layer="20"/>
<wire x1="-1.27" y1="64.77" x2="26.67" y2="64.77" width="0.2032" layer="20"/>
<wire x1="-0.254" y1="43.18" x2="-1.27" y2="44.45" width="0.2032" layer="20"/>
<wire x1="-1.27" y1="44.45" x2="-1.27" y2="64.77" width="0.2032" layer="20"/>
<text>Teensy &gt; FIO Translate Board</text>
<text>v0.1</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X14">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-1">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH">
</package>
</packages>
</library>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1+4">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="custom_components">
<packages>
<package name="SOT95P300X145-5N">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="TeUbi.co">
<packages>
<package name="LOGOVECTOR2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X14" value="M14"/>
<element name="JP5" library="SparkFun" package="1X14" value="M14"/>
<element name="U$2" library="SparkFun-RF" package="XBEE-1" value="XBEE-1B1"/>
<element name="JP4" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2"/>
<element name="U$1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1+4" value="TEENSY_3.1+4"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="IC1" library="custom_components" package="SOT95P300X145-5N" value="MCP73831T-2ATI/OT">
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="OC_NEWARK" value="84R5196"/>
<attribute name="MPN" value="MCP73831T-2ATI/OT"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1834890"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="U$3" library="TeUbi.co" package="LOGOVECTOR2" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="AGND"/>
<contactref element="U$2" pad="10"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="14"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="13"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="RXI">
<contactref element="JP5" pad="4"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="0"/>
</signal>
<signal name="TXO">
<contactref element="JP5" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="D2">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="D3">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="D4">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="D5">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="D6">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="D8">
<contactref element="JP1" pad="9"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="D10">
<contactref element="JP1" pad="11"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="A0">
<contactref element="JP5" pad="7"/>
<contactref element="U$1" pad="14/A0"/>
</signal>
<signal name="A1">
<contactref element="JP5" pad="8"/>
<contactref element="U$1" pad="15/A1"/>
</signal>
<signal name="A2">
<contactref element="JP5" pad="9"/>
<contactref element="U$1" pad="16/A2"/>
</signal>
<signal name="A3">
<contactref element="JP5" pad="10"/>
<contactref element="U$1" pad="17/A3"/>
</signal>
<signal name="A4">
<contactref element="JP5" pad="11"/>
<contactref element="U$1" pad="18/A4"/>
</signal>
<signal name="A5">
<contactref element="JP5" pad="12"/>
<contactref element="U$1" pad="19/A5"/>
</signal>
<signal name="D7">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D9">
<contactref element="JP1" pad="10"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="A6">
<contactref element="JP5" pad="13"/>
<contactref element="U$1" pad="20/A6"/>
</signal>
<signal name="A7">
<contactref element="JP5" pad="14"/>
<contactref element="U$1" pad="21/A7"/>
</signal>
<signal name="AREF">
<contactref element="JP5" pad="2"/>
<contactref element="U$1" pad="AREF"/>
</signal>
<signal name="A8">
<contactref element="JP5" pad="6"/>
<contactref element="U$1" pad="22/A8"/>
</signal>
<signal name="VBAT">
<contactref element="U$1" pad="VBAT"/>
</signal>
<signal name="VUSB">
<contactref element="IC1" pad="4"/>
<contactref element="LED1" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="VUSB"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="JP5" pad="3"/>
<contactref element="U$1" pad="3.3V1"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="JP4" pad="2"/>
<contactref element="U$1" pad="VIN"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
