<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.02" y2="0" width="0.2032" layer="20"/>
<wire x1="33.02" y1="25.4" x2="0" y2="25.4" width="0.2032" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="17.145" width="0.2032" layer="20"/>
<wire x1="0" y1="17.145" x2="2.286" y2="17.145" width="0.2032" layer="20"/>
<wire x1="2.286" y1="17.145" x2="2.286" y2="8.255" width="0.2032" layer="20"/>
<wire x1="2.286" y1="8.255" x2="0" y2="8.255" width="0.2032" layer="20"/>
<wire x1="0" y1="8.255" x2="0" y2="0" width="0.2032" layer="20"/>
<text>SPKR_R</text>
<text>SPKR_L</text>
<text>LED1</text>
<text>LED0</text>
<text>TXO</text>
<text>RXI</text>
<text>CTS</text>
<text>3.3V</text>
<text>RTS</text>
<text>GND</text>
<text>PWREN</text>
<text>All Dimensions in mm</text>
<text>29-7-13</text>
<wire x1="33.02" y1="25.4" x2="33.02" y2="0" width="0.254" layer="20"/>
<text>v1.2</text>
<text>CMD</text>
<text>MIC_L</text>
<text>MIC_R</text>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RN-52">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="analog-devices">
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;10-Lead Mini Small Outline Package [MSOP]&lt;/b&gt; (RM-10)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/35641221898805SSM2167_b.pdf&lt;br&gt;
COMPLIANT TO JEDEC STANDARDS MO-187BA</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="SparkFun-RF" package="RN-52" value="BLUETOOTH-RN-52"/>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="470"/>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="470"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="C1" library="SparkFun-Passives" package="0402-CAP" value="47nF"/>
<element name="C2" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="C3" library="SparkFun-Passives" package="0402-CAP" value="47nF"/>
<element name="C4" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="C5" library="SparkFun-Passives" package="0402-CAP" value="47nF"/>
<element name="C6" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="C7" library="SparkFun-Passives" package="0402-CAP" value="47nF"/>
<element name="C8" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="C9" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="2K2"/>
<element name="R4" library="SparkFun-Passives" package="0402-RES" value="2K2"/>
<element name="R5" library="SparkFun-Passives" package="0402-RES" value="22K"/>
<element name="R6" library="SparkFun-Passives" package="0402-RES" value="22k"/>
<element name="R7" library="SparkFun-Passives" package="0402-RES" value="22k"/>
<element name="R8" library="SparkFun-Passives" package="0402-RES" value="22k"/>
<element name="R9" library="SparkFun-Passives" package="0402-RES" value="47k"/>
<element name="R10" library="SparkFun-Passives" package="0402-RES" value="47k"/>
<element name="R11" library="SparkFun-Passives" package="0402-RES" value="47k"/>
<element name="R12" library="SparkFun-Passives" package="0402-RES" value="47k"/>
<element name="C11" library="SparkFun-Passives" package="0402-CAP" value="1uF"/>
<element name="IC2" library="analog-devices" package="MSOP10" value="TPA6112A2">
<attribute name="OC_NEWARK" value="31M4422"/>
<attribute name="MPN" value="AD7992BRMZ-0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1078311"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="C15" library="SparkFun-Passives" package="0805" value="100uF"/>
<element name="C16" library="SparkFun-Passives" package="0805" value="100uF"/>
<element name="C17" library="SparkFun-Passives" package="0805" value="100uF"/>
<element name="C18" library="SparkFun-Passives" package="0805" value="100uF"/>
<element name="SPKR" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="MIC" library="SparkFun-Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="RFG1"/>
<contactref element="U$2" pad="RFG2"/>
<contactref element="U$2" pad="RFG3"/>
<contactref element="U$2" pad="RFG4"/>
<contactref element="U$2" pad="RFG5"/>
<contactref element="U$2" pad="RFG6"/>
<contactref element="U$2" pad="G4"/>
<contactref element="U$2" pad="G3"/>
<contactref element="U$2" pad="G2"/>
<contactref element="U$2" pad="G1"/>
<contactref element="U$2" pad="36"/>
<contactref element="C2" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="5"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PWREN">
<contactref element="U$2" pad="19"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="20"/>
<contactref element="U$2" pad="17"/>
<contactref element="IC2" pad="10"/>
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LED1">
<contactref element="U$2" pad="29"/>
<contactref element="JP2" pad="4"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="LED0">
<contactref element="U$2" pad="30"/>
<contactref element="JP2" pad="3"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="MIC_BIAS">
<contactref element="U$2" pad="31"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="MIC_L+">
<contactref element="U$2" pad="32"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="MIC_R+">
<contactref element="U$2" pad="33"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="MIC_L-">
<contactref element="U$2" pad="34"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="MIC_R-">
<contactref element="U$2" pad="35"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="SPKR_R">
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="SPKR" pad="2"/>
</signal>
<signal name="SPKR_L">
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="SPKR" pad="1"/>
</signal>
<signal name="MIC_R">
<contactref element="C7" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="MIC" pad="2"/>
</signal>
<signal name="MIC_L">
<contactref element="C5" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="MIC" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="U$2" pad="14"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RTS">
<contactref element="U$2" pad="13"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="TXO">
<contactref element="U$2" pad="15"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RXI">
<contactref element="U$2" pad="16"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C8" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C9" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SPKR_L+">
<contactref element="C6" pad="1"/>
<contactref element="U$2" pad="40"/>
</signal>
<signal name="SPKR_R+">
<contactref element="C8" pad="1"/>
<contactref element="U$2" pad="39"/>
</signal>
<signal name="SPKR_R-">
<contactref element="C9" pad="1"/>
<contactref element="U$2" pad="37"/>
</signal>
<signal name="N$17">
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R7" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R12" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="R12" pad="1"/>
<contactref element="IC2" pad="9"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="SPKR_L-">
<contactref element="C4" pad="1"/>
<contactref element="U$2" pad="38"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$10">
</signal>
<signal name="N$15">
</signal>
<signal name="N$20">
</signal>
<signal name="N$23">
</signal>
<signal name="N$14">
</signal>
<signal name="N$24">
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$25">
</signal>
<signal name="MCMD">
<contactref element="JP2" pad="5"/>
<contactref element="U$2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
