<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="34.798" y2="0" width="0" layer="20"/>
<wire x1="34.798" y1="0" x2="34.798" y2="58.41" width="0" layer="20"/>
<wire x1="34.798" y1="58.41" x2="0" y2="58.41" width="0" layer="20"/>
<wire x1="0" y1="58.41" x2="0" y2="0" width="0" layer="20"/>
<hole x="4.445" y="53.975" drill="5.9436"/>
<hole x="30.48" y="4.445" drill="5.9436"/>
<hole x="4.445" y="4.445" drill="5.9436"/>
<hole x="30.48" y="53.975" drill="5.9436"/>
<text>+5</text>
<text>+12</text>
<text>12</text>
<text>12</text>
<text>12</text>
<text>5</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>5</text>
<text>G</text>
<text>IN</text>
<text>OUT</text>
<text>F1:</text>
<text>F2:</text>
<text>G</text>
<text>5</text>
<text>12</text>
<text>MOD</text>
</plain>
<libraries>
<library name="connectors">
<packages>
<package name="KK-156-10">
<description>&lt;b&gt;KK 156 HEADER&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/026604100_sd.pdf</description>
</package>
<package name="KK-156-4">
<description>&lt;b&gt;KK 156 HEADER&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/026604100_sd.pdf</description>
</package>
<package name="MOLEX10-09-1033">
</package>
</packages>
</library>
<library name="fuses">
<packages>
<package name="BK/1A4534-06-X2-WFUSE">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="connectors" package="KK-156-10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="connectors" package="KK-156-4" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fuses" package="BK/1A4534-06-X2-WFUSE" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fuses" package="BK/1A4534-06-X2-WFUSE" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="150"/>
<element name="R2" library="SparkFun-Resistors" package="1206" value="510"/>
<element name="U$3" library="connectors" package="MOLEX10-09-1033" value="MOLEX10-09-1033"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="X2" pad="4"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="LED2" pad="A"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="LED1" pad="A"/>
<contactref element="X1" pad="4"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="P$5"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="3"/>
<contactref element="X1" pad="10"/>
<contactref element="X1" pad="8"/>
<contactref element="X1" pad="7"/>
<contactref element="X1" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="P$3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
