<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="41.91" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0.2032" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="41.91" width="0.2032" layer="20"/>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>GND</text>
<text>RST</text>
<text>VC</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<wire x1="0" y1="41.91" x2="25.4" y2="41.91" width="0.254" layer="20"/>
<text>A5</text>
<text>A4</text>
<hole x="12.7" y="2.54" drill="3.2"/>
<hole x="22.86" y="31.75" drill="3.2"/>
<text>SCL</text>
<text>SDA</text>
<text>I2C:</text>
<text>Temp/Hum
SHT21</text>
<text>Compass
HMC5883</text>
<text>XAmbi Node Pro
Frank Herrmann
V0.1 Xpix
Jul 2015 / Beta</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="16LPCC">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="_adafruit">
<packages>
<package name="1X10-BIG">
</package>
<package name="1X08-CLEANBIG">
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Misenso">
<packages>
<package name="SEN-SENSIRION-SHT2X">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="_xpix">
<packages>
<package name="NRF24L01_1.27">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="RFM12B-ANTENNA">
</package>
<package name="RFM69W-MINPADS">
</package>
<package name="RFM12B-MINPADS">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_20MM_4LEGS" value="20mm coincell">
<attribute name="PROD_ID" value="BATT-10373"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="U$1" library="_adafruit" package="1X10-BIG" value="PINHD-1X10"/>
<element name="SHT21" library="Misenso" package="SEN-SENSIRION-SHT2X" value="SHT21"/>
<element name="JP2" library="_adafruit" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="_adafruit" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="_adafruit" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="_adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="_adafruit" package="1X10-BIG" value="PINHD-1X10"/>
<element name="IC2" library="microchip" package="SO-08" value="AT25DF512C-SSHN-B">
<attribute name="OC_NEWARK" value="92C7351"/>
<attribute name="MPN" value="25AA080/SN"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1816072"/>
</element>
<element name="DASDD" library="_xpix" package="NRF24L01_1.27" value="NRF24L01+_1.27"/>
<element name="JP5" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="U$4" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="RFM69W" library="LowPowerLab" package="RFM69W-MINPADS" value="RFM69">
<attribute name="NAME"/>
</element>
<element name="RFM12B" library="LowPowerLab" package="RFM12B-MINPADS" value="RFM12B_MINPADS">
<attribute name="NAME"/>
</element>
<element name="U2" library="SparkFun" package="16LPCC" value="HMC5883LSMD">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="0603-CAP" value=".22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="0603-CAP" value="4.7uF"/>
<element name="R3" library="SparkFun" package="0603-RES" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0603-RES" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="BAT1" pad="2"/>
<contactref element="SHT21" pad="2"/>
<contactref element="SHT21" pad="7"/>
<contactref element="GND" pad="3"/>
<contactref element="GND" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="U$3" pad="9"/>
<contactref element="IC2" pad="4"/>
<contactref element="DASDD" pad="P$7"/>
<contactref element="RFM69W" pad="GND"/>
<contactref element="RFM12B" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="RESET">
<contactref element="U$3" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="BAT1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="SHT21" pad="5"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="DASDD" pad="P$8"/>
<contactref element="RFM69W" pad="VDD"/>
<contactref element="RFM12B" pad="VDD"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="DASDD" pad="P$6"/>
</signal>
<signal name="D8">
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="D2">
<contactref element="JP2" pad="8"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP4" pad="8"/>
<contactref element="U$3" pad="8"/>
<contactref element="DASDD" pad="P$1"/>
<contactref element="RFM69W" pad="DIO0"/>
<contactref element="RFM12B" pad="IRQ"/>
</signal>
<signal name="D3">
<contactref element="JP4" pad="7"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP2" pad="7"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="D4">
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP4" pad="6"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="D5">
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP4" pad="5"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="D6">
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="D7">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="IC2" pad="6"/>
<contactref element="DASDD" pad="P$4"/>
<contactref element="RFM69W" pad="SCK"/>
<contactref element="RFM12B" pad="SCK"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="8"/>
<contactref element="IC2" pad="2"/>
<contactref element="DASDD" pad="P$2"/>
<contactref element="RFM69W" pad="MISO"/>
<contactref element="RFM12B" pad="SDO"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="9"/>
<contactref element="IC2" pad="5"/>
<contactref element="DASDD" pad="P$3"/>
<contactref element="RFM69W" pad="MOSI"/>
<contactref element="RFM12B" pad="SDI"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="5"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="6"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="10"/>
<contactref element="DASDD" pad="P$5"/>
<contactref element="RFM69W" pad="NSS"/>
<contactref element="RFM12B" pad="SEL"/>
</signal>
<signal name="A5_SCL">
<contactref element="JP1" pad="1"/>
<contactref element="SHT21" pad="6"/>
<contactref element="JP5" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="A4_SDA">
<contactref element="JP1" pad="2"/>
<contactref element="SHT21" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$4" pad="P$1"/>
<contactref element="RFM69W" pad="ANA"/>
<contactref element="RFM12B" pad="ANT"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="8"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="12"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="10"/>
<contactref element="C5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
