<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="52.07" y2="44.45" width="0" layer="20"/>
<wire x1="52.07" y1="44.45" x2="52.07" y2="80" width="0" layer="20"/>
<wire x1="52.07" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="44.45" width="0" layer="20"/>
<hole x="43.18" y="74.93" drill="3.2"/>
<hole x="43.18" y="49.53" drill="3.2"/>
<text>A1</text>
<text>A2</text>
<text>G1</text>
<text>G2</text>
<text>C1</text>
<text>C2</text>
<text>CT</text>
<text>H1</text>
<text>H2</text>
<text>DUAL TRIODE
ADAPTOR BOARD</text>
<text>TRIODE #1</text>
<text>TRIODE #2</text>
<text>CT</text>
<text>H2</text>
<text>H1</text>
<text>TJP 6/2014</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>4</text>
<text>5</text>
<text>9</text>
<text>CT</text>
<text>9</text>
<text>1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
</packages>
</library>
<library name="belton-engineering">
<description>&lt;b&gt;Belton Engineering Co., Ltd.&lt;/b&gt;&lt;p&gt;
Unit 1208, Daerung Techno town 8&lt;br&gt;
481-11, Gasan-Dong&lt;br&gt;
Geumcheon-Gu, Seoul, Korea&lt;br&gt;
E-mail :&amp;lt;belton@unitel.co.kr&amp;gt;&lt;p&gt;
 
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VT9-PT">
<description>&lt;b&gt;VACUUM TUBE SOCKET&lt;/b&gt;&lt;p&gt;
Source: 00004280-VT9-PT.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="SX1" library="belton-engineering" package="VT9-PT" value="VT9-PT"/>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="SX1" pad="9"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="SX1" pad="8"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="3"/>
<contactref element="SX1" pad="7"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="SX1" pad="6"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="SX1" pad="5"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="6"/>
<contactref element="SX1" pad="4"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="7"/>
<contactref element="SX1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="8"/>
<contactref element="SX1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="9"/>
<contactref element="SX1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
</signals>
</board>
</drawing>
</eagle>
