<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<hole x="32.4" y="34.2" drill="1"/>
<hole x="34.9" y="34.2" drill="1"/>
<hole x="41.2" y="34.2" drill="1"/>
<hole x="43.8" y="34.2" drill="1"/>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="theairboard">
<description>&lt;h3&gt;The AirBoard®&lt;/h3&gt; is a thumb-size, Arduino-compatible, wireless,
ubiquitous computer designed to sketch Internet-of-Things, fast!
&lt;br&gt;&lt;br&gt;
Visit &lt;b&gt;http://www.theairboard.cc&lt;/b&gt;</description>
<packages>
<package name="SIL-1X10">
<description>&lt;b&gt;Single In Line 2.54mm header - 10 pins&lt;/b&gt;</description>
</package>
<package name="BOARD_FRAME">
<description>&lt;b&gt;Board frame&lt;/b&gt;</description>
</package>
<package name="SC70-6">
</package>
<package name="LAYOUT25X25">
<description>25x25mm board template</description>
</package>
<package name="DO-214AC">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="DESIGNER" value="theairboard.cc"/>
<attribute name="REV" value="1.0"/>
<attribute name="SENSOR" value="Dual motor drive"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="theairboard" package="SIL-1X10" value="SIL">
<attribute name="OC_NEWARK" value="93K5133"/>
<attribute name="MANUFACTURER" value="FCI"/>
<attribute name="OC_FARNELL" value="1097958"/>
<attribute name="PART_NUMBER" value="77315-818-36LF "/>
</element>
<element name="FRAME1" library="theairboard" package="BOARD_FRAME" value="SCH_FRAME"/>
<element name="M1" library="theairboard" package="SC70-6" value="FDG6303N">
<attribute name="DESCRIPTION" value="Dual N-Channel, Digital FET"/>
<attribute name="MANUFACTURER" value="FAIRCHILD"/>
<attribute name="PART_NUMBER" value="FDG6303N"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="theairboard" package="LAYOUT25X25" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="JP3" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="JP4" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="JP5" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="D1" library="theairboard" package="DO-214AC" value="S1M">
<attribute name="OC_NEWARK" value="58K2390"/>
<attribute name="MANUFACTURER" value="Fairchild"/>
<attribute name="OC_FARNELL" value="9843841"/>
<attribute name="PART_NUMBER" value="S1M"/>
</element>
<element name="D2" library="theairboard" package="DO-214AC" value="S1M">
<attribute name="OC_NEWARK" value="58K2390"/>
<attribute name="MANUFACTURER" value="Fairchild"/>
<attribute name="OC_FARNELL" value="9843841"/>
<attribute name="PART_NUMBER" value="S1M"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="7"/>
<contactref element="M1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="8"/>
<contactref element="M1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP4" pad="1"/>
<contactref element="M1" pad="6"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="M1" pad="3"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP3" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
