<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="14.859" width="0.2032" layer="20"/>
<wire x1="0" y1="14.859" x2="16.1544" y2="14.859" width="0.2032" layer="20"/>
<wire x1="16.1544" y1="14.859" x2="16.129" y2="0" width="0.2032" layer="20"/>
<wire x1="16.129" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>3.3V</text>
<text>SDA</text>
<text>SCL</text>
<text>I2</text>
<text>I1</text>
<text>GND</text>
<text>MMA8452</text>
<text>X</text>
<text>Y</text>
<text>Z</text>
<text>SA0
Open 0x1D
Closed 0x1C</text>
<text>3.3V</text>
<text>SDA</text>
<text>SCL</text>
<text>I2</text>
<text>I1</text>
<text>GND</text>
<text>v3 12-16-14
chip@mcclellands.org</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X06">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-16_0.5MM">
<description>&lt;h3&gt;QFN-16 0.5mm Pitch&lt;/h3&gt;
3 x 3mm Outline&lt;br&gt;
16-pin&lt;br&gt;
Used on the MMA8452Q accelerometer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Layout in accordance with App note AN4077&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/app_note/AN4077.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-Sensors" package="QFN-16_0.5MM" value="MMA8452Q">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="IC-10769"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="1X06" value="Header"/>
<element name="SA0" library="SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP1" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
</elements>
<signals>
<signal name="BYP">
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="12"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP5" pad="6"/>
<contactref element="SA0" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="INT2">
<contactref element="U1" pad="9"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="INT1">
<contactref element="U1" pad="11"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="SA0">
<contactref element="U1" pad="7"/>
<contactref element="SA0" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
