<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="21.59" y2="1.27" width="0" layer="20"/>
<wire x1="21.59" y1="1.27" x2="21.59" y2="24.13" width="0" layer="20"/>
<wire x1="21.59" y1="24.13" x2="0" y2="24.13" width="0" layer="20"/>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0" layer="20"/>
<text>POT</text>
<text>MIC</text>
<text>BOARD</text>
<text>LM386</text>
<text>10uF</text>
<text>1K</text>
<text>.01uF</text>
<text>7/15/2012</text>
</plain>
<libraries>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH">
</package>
<package name="JST-3-PTH">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-AnalogIC" package="DIP08" value="LM386"/>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-PTH" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="JST-2-PTH" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="C2" library="SparkFun-Passives" package="0805" value=".01uF"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="1K"/>
<element name="C1" library="SparkFun-Passives" package="EIA3216" value="10uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP3" pad="3"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="C"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="6"/>
<contactref element="JP3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
