<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.31" y2="0" width="0" layer="20"/>
<wire x1="40.31" y1="0" x2="40.31" y2="38.09" width="0" layer="20"/>
<wire x1="40.31" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="Johns">
<packages>
<package name="6MM_ILL_SWT">
<description>Illuminated 6mm tact switch w/ 10mm rnd cap options</description>
</package>
<package name="3362">
</package>
<package name="0204/3">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D" library="Johns" package="6MM_ILL_SWT" value="TSL06122THM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="JP1" library="adafruit" package="1X03" value="BUTT"/>
<element name="L" library="Johns" package="6MM_ILL_SWT" value="TSL06122THM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="R" library="Johns" package="6MM_ILL_SWT" value="TSL06122THM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="R1" library="Johns" package="0204/3" value="2K">
<attribute name="OC_NEWARK" value="38K5177"/>
<attribute name="MPN" value="MF50 2K"/>
<attribute name="MF" value="FARNELL"/>
</element>
<element name="R10" library="Johns" package="0204/3" value="68">
<attribute name="OC_NEWARK" value="98K3817"/>
<attribute name="MPN" value="YR1B45R3CC"/>
<attribute name="MF" value=""/>
</element>
<element name="R2" library="Johns" package="0204/3" value="330">
<attribute name="OC_NEWARK" value="38K0292"/>
<attribute name="MPN" value="MCF 0.5W 330R"/>
<attribute name="MF" value="FARNELL"/>
</element>
<element name="R3" library="Johns" package="0204/3" value="620">
<attribute name="OC_NEWARK" value="38K5239"/>
<attribute name="MPN" value="MF50 620R"/>
<attribute name="MF" value="FARNELL"/>
</element>
<element name="R4" library="Johns" package="0204/3" value="1K">
<attribute name="OC_NEWARK" value="38K0327"/>
<attribute name="MPN" value="MCF 0.25W 1K"/>
<attribute name="MF" value="FARNELL"/>
</element>
<element name="R5" library="Johns" package="0204/3" value="3.3K">
<attribute name="OC_NEWARK" value="33C4569"/>
<attribute name="MPN" value="EW233"/>
<attribute name="MF" value=""/>
</element>
<element name="R6" library="Johns" package="0204/3" value="68">
<attribute name="OC_NEWARK" value="98K3817"/>
<attribute name="MPN" value="YR1B45R3CC"/>
<attribute name="MF" value=""/>
</element>
<element name="R7" library="Johns" package="0204/3" value="68">
<attribute name="OC_NEWARK" value="98K3817"/>
<attribute name="MPN" value="YR1B45R3CC"/>
<attribute name="MF" value=""/>
</element>
<element name="R8" library="Johns" package="0204/3" value="68">
<attribute name="OC_NEWARK" value="98K3817"/>
<attribute name="MPN" value="YR1B45R3CC"/>
<attribute name="MF" value=""/>
</element>
<element name="R9" library="Johns" package="0204/3" value="68">
<attribute name="OC_NEWARK" value="98K3817"/>
<attribute name="MPN" value="YR1B45R3CC"/>
<attribute name="MF" value=""/>
</element>
<element name="SEL" library="Johns" package="6MM_ILL_SWT" value="TSL06122THM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="U" library="Johns" package="6MM_ILL_SWT" value="TSL06122THM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H3" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H5" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H6" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="TM1" library="Johns" package="3362" value=""/>
<element name="POT" library="adafruit" package="1X03" value="10K_LCD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="R1" pad="1"/>
<contactref element="R" pad="1"/>
<contactref element="U" pad="1"/>
<contactref element="D" pad="1"/>
<contactref element="L" pad="1"/>
<contactref element="SEL" pad="1"/>
<contactref element="SEL" pad="2"/>
<contactref element="L" pad="2"/>
<contactref element="D" pad="2"/>
<contactref element="U" pad="2"/>
<contactref element="R" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="SEL" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="SEL" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="L" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="L" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="D" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="D" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="U" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R10" pad="1"/>
<contactref element="SEL" pad="+"/>
</signal>
<signal name="N$2">
<contactref element="R9" pad="1"/>
<contactref element="L" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="1"/>
<contactref element="D" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="1"/>
<contactref element="U" pad="+"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="R" pad="+"/>
</signal>
<signal name="GND">
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R" pad="-"/>
<contactref element="U" pad="-"/>
<contactref element="D" pad="-"/>
<contactref element="L" pad="-"/>
<contactref element="SEL" pad="-"/>
<contactref element="R" pad="4"/>
<contactref element="R" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="TM1" pad="P$1"/>
<contactref element="POT" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="R10" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="TM1" pad="P$3"/>
<contactref element="POT" pad="1"/>
</signal>
<signal name="VO">
<contactref element="TM1" pad="P$2"/>
<contactref element="POT" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
