<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.7" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="12.7" y2="9.9" width="0" layer="20"/>
<wire x1="12.7" y1="9.9" x2="0" y2="9.9" width="0" layer="20"/>
<wire x1="0" y1="9.9" x2="0" y2="0" width="0" layer="20"/>
<hole x="1.2" y="8.7" drill="2"/>
<hole x="11.5" y="8.7" drill="2"/>
<text>+Y</text>
<text>+X</text>
<text>+Z</text>
<text>INT</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>1.8-3.3V</text>
</plain>
<libraries>
<library name="QuadLib">
<packages>
<package name="24QFN3X3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X2" library="QuadLib" package="24QFN3X3" value="MPU6500"/>
<element name="X2C1" library="SparkFun-Passives" package="0402-CAP" value=".1uF,10%,4v">
<attribute name="NAME"/>
</element>
<element name="X2C3" library="SparkFun-Passives" package="0402-CAP" value="10nF,10%,4v">
<attribute name="NAME"/>
</element>
<element name="X2C2" library="SparkFun-Passives" package="0402-CAP" value=".1uF,10%,2V">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X2" pad="11"/>
<contactref element="X2C1" pad="1"/>
<contactref element="X2C3" pad="1"/>
<contactref element="X2" pad="18"/>
<contactref element="X2" pad="20"/>
<contactref element="X2C2" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="X2" pad="9"/>
</signal>
<signal name="I2C_SCL">
<contactref element="X2" pad="23"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="I2C_SDA">
<contactref element="X2" pad="24"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="INT_XLA">
<contactref element="X2" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="X2C1" pad="2"/>
<contactref element="X2" pad="10"/>
</signal>
<signal name="3.2V">
<contactref element="X2" pad="13"/>
<contactref element="X2C2" pad="2"/>
<contactref element="X2" pad="8"/>
<contactref element="X2C3" pad="2"/>
<contactref element="X2" pad="22"/>
<contactref element="JP1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
